(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "+1V1")
  (net 2 "+3.3V")
  (net 3 "RST")
  (net 4 "VBUS")
  (net 5 "GND")
  (net 6 "VSYS")
  (net 7 "GPIO26")
  (net 8 "GPIO27")
  (net 9 "GPIO28")
  (net 10 "GPIO15")
  (net 11 "GPIO14")
  (net 12 "GPIO16")
  (net 13 "GPIO00")
  (net 14 "GPIO01")
  (net 15 "GPIO02")
  (net 16 "GPIO03")
  (net 17 "GPIO04")
  (net 18 "GPIO05")
  (net 19 "GPIO06")
  (net 20 "GPIO07")
  (net 21 "GPIO08")
  (net 22 "GPIO09")
  (net 23 "GPIO10")
  (net 24 "GPIO11")
  (net 25 "GPIO12")
  (net 26 "GPIO13")
  (net 27 "AREF")
  (net 28 "Net-(C3-Pad1)")
  (net 29 "Net-(C1-Pad2)")
  (net 30 "Net-(C16-Pad1)")
  (net 31 "Net-(C16-Pad2)")
  (net 32 "Net-(D4-Pad2)")
  (net 33 "GPIO17")
  (net 34 "GPIO18")
  (net 35 "GPIO19")
  (net 36 "Net-(J7-PadA5)")
  (net 37 "DP")
  (net 38 "unconnected-(J7-PadA8)")
  (net 39 "Net-(J7-PadB5)")
  (net 40 "unconnected-(J7-PadB8)")
  (net 41 "GPIO20")
  (net 42 "GPIO21")
  (net 43 "GPIO22")
  (net 44 "GPIO23")
  (net 45 "GPIO24")
  (net 46 "GPIO25")
  (net 47 "SWCLK")
  (net 48 "SWD")
  (net 49 "Net-(C2-Pad2)")
  (net 50 "Net-(R4-Pad1)")
  (net 51 "QSPI_SS")
  (net 52 "3,3V_EN")
  (net 53 "D+")
  (net 54 "D-")
  (net 55 "QSPI_SD3")
  (net 56 "QSPI_SCLK")
  (net 57 "QSPI_SD0")
  (net 58 "QSPI_SD2")
  (net 59 "QSPI_SD1")
  (net 60 "VBUSPIN")
  (net 61 "Net-(R1-Pad1)")
  (net 62 "GND1")
  (net 63 "Net-(D5-Pad1)")
  (net 64 "Net-(D2-Pad1)")
  (net 65 "Net-(D3-Pad1)")
  (net 66 "GPIO29")
  (net 67 "unconnected-(J7-PadS1)")
  (net 68 "DN")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.674 119.801 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "470Ω" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 163.5 112.5 180)
    (descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "W25Q16JVSSIQ" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.6 -1.905 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "QSPI_SS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -3.6 -0.635 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "QSPI_SD1") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.6 0.635 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "QSPI_SD2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.6 1.905 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 3.6 1.905 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "QSPI_SD0") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 3.6 0.635 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "QSPI_SCLK") (pinfunction "CLK") (pintype "input"))
    (pad "7" smd roundrect (at 3.6 -0.635 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "QSPI_SD3") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 3.6 -1.905 180) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.275x5.275mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.949 84.226 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "20pf" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.274 106.751 -135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43 -135) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 -135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 225) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 225) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 155.15 66.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.2 77.05 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "470Ω" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.224 98.851 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "GPIO24") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm" (layer "F.Cu")
    (tedit 627AC11D)
    (at 155 101.75 -135)
    (descr "QFN, 56 Pin (https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf#page=634), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.82 45) (layer "F.SilkS") hide)
    (fp_text value "RP2040" (at 0 4.82 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.8 0.8 225) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.1937976744))
    (pad "" smd roundrect (at 0.8 -0.8 225) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.1937976744))
    (pad "" smd roundrect (at -0.8 0.8 225) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.1937976744))
    (pad "" smd roundrect (at -0.8 -0.8 225) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.1937976744))
    (pad "1" smd roundrect (at -3.4375 -2.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.4375 -2.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "GPIO00") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.8 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GPIO01") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.4 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GPIO02") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -1 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "GPIO03") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.4375 -0.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "GPIO04") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.4375 -0.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "GPIO05") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "GPIO06") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 0.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "GPIO07") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "11" smd roundrect (at -3.4375 1.4 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "GPIO08") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 1.8 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "GPIO09") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.4375 2.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GPIO10") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.4375 2.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "GPIO11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "GPIO12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GPIO13") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "GPIO14") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -1.4 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "GPIO15") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -1 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "TESTEN") (pintype "input"))
    (pad "20" smd roundrect (at -0.6 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(C1-Pad2)") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R1-Pad1)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "23" smd roundrect (at 0.6 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "SWD") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "RST") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "GPIO16") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 2.6 3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "GPIO17") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 2.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "GPIO18") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 2.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "GPIO19") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 1.8 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GPIO20") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 1.4 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "GPIO21") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 1 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "34" smd roundrect (at 3.4375 0.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "GPIO22") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 0.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "GPIO23") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 3.4375 -0.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "GPIO24") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.4375 -0.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "GPIO25") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.4375 -1 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GPIO26") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.4375 -1.4 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "GPIO27") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.4375 -1.8 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "GPIO28") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 3.4375 -2.2 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GPIO29") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.4375 -2.6 225) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "43" smd roundrect (at 2.6 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "AREF") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "DN") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "DP") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "50" smd roundrect (at -0.2 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pinfunction "DVDD") (pintype "passive"))
    (pad "51" smd roundrect (at -0.6 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "QSPI_SD3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "QSPI_SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "QSPI_SD0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "QSPI_SD2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "QSPI_SD1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.4375 225) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "QSPI_SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" smd rect (at 0 0 225) (size 3.2 3.2) (layers "F.Cu" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.824 109.201 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43 45) (layer "F.SilkS") hide)
    (fp_text value "2,2µf" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 45) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 45) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.5 68.75 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "Varistor" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.375 89.65 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "27Ω" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "DN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "F.Cu")
    (tedit 5B61DEEA)
    (at 153.851 71.85 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 0 -4.6 90) (layer "F.SilkS") hide)
    (fp_text value "3,9µH" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(C16-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3.3V") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A431)
    (at 135.96 115.32 90)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x09" (at 0 23.09 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 10.16) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "GPIO17") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "GPIO18") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "GPIO19") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "GPIO20") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "GPIO21") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "GPIO22") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "GPIO23") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "GPIO24") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "GPIO25") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.824 71.001 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "1nf" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.724 119.801 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 164.25 65.3 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J7-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.23 98.851 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "2kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "AREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "F.Cu")
    (tedit 5CA1CA7F)
    (at 166.624 87.951 90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 0 180) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 4.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.05 90) (layer "F.Fab"))
    (pad "1" smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R4-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R4-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 168.95 77.05 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "470Ω" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 171.2 80.9 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "LED_YELLOW" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GPIO13") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.224 86 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "RST") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 136 66.25 -90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J6" (at -8.45 5.75 90) (layer "F.SilkS") hide)
    (fp_text value "Barrel_Jack_MountingPin" (at -6.4 -4.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 6 "VSYS") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill 2.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 62 "GND1") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "${KIPRJMOD}/barrel_jack.stp"
      (offset (xyz -5.75 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "F.Cu")
    (tedit 5CA1CA7F)
    (at 177 60.75 90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at 0 -4.05 90) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 4.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.05 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "RST") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "RST") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156 63.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "3,3V_EN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.5 65.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J7-PadA5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 164.224 116.501 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43 180) (layer "F.SilkS") hide)
    (fp_text value "LED_GREEN_PWR" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.924 112 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "2,2µf" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.52 97.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162.424 94.601)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.375 89.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "27Ω" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "DP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "D+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 164.4 71.8 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.75 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 180) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 53 "D+") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 136.55 76.0495 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "PJA3432AU" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(D5-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "GND1") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tedit 58641739)
    (at 137.5 71.587 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.85 90) (layer "F.SilkS") hide)
    (fp_text value "~7v Zener" (at 0.1 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.574 71.001 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 158.824 67.001 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.4 -90) (layer "F.SilkS") hide)
    (fp_text value "PJA3432AU" (at 0 2.4 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GPIO29") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C3-Pad1)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 139.324 102.751 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 2.625 0.02 180) (layer "F.SilkS") hide)
    (fp_text value "LM4040DBZ-3" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "AREF") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "A") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.224 95.401 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "5,6kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "VBUSPIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "GPIO24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.574 66.801 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "200kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:WAGO SMD terminal, 2P 4mm" (layer "F.Cu")
    (tedit 0)
    (at 145.7 62.05)
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 -3 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 -7.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -9.25 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 5.5 90) (size 3.5 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "GND1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" smd roundrect (at -2 -3.75 90) (size 6 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "GND1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 5.5 90) (size 3.5 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" smd roundrect (at 2 -3.75 90) (size 6 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/wago.stp"
      (offset (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162.624 102.101 -45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43 -45) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 -45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 315) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 315) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_4x4.5" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 153 60.45 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -3.2 90) (layer "F.SilkS") hide)
    (fp_text value "10µf" (at 0 3.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 6 "VSYS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x4.5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.524 95.501)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-6" (layer "F.Cu")
    (tedit 5F6F97DB)
    (at 152.351 66.1 -90)
    (descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "AP63203WU" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pinfunction "FB") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "3,3V_EN") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pinfunction "IN") (pintype "power_in"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 0 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(C16-Pad2)") (pinfunction "SW") (pintype "output"))
    (pad "6" smd roundrect (at 1.1375 -0.95 270) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(C16-Pad1)") (pinfunction "BST") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.424 116.401)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "2,2µf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.924 112 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.949 80.776 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "20pf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 159 61.75 -90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.82 90) (layer "F.SilkS") hide)
    (fp_text value "500mA" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 60 "VBUSPIN") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 4 "VBUS") (pintype "passive"))
    (model "${KIPRJMOD}/fuse.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_4x4.5" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 143.15 72.95 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -3.2 90) (layer "F.SilkS") hide)
    (fp_text value "22µf" (at 0 3.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x4.5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_4x4.5" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 148.15 72.95 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -3.2 90) (layer "F.SilkS") hide)
    (fp_text value "22µf" (at 0 3.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x4.5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_7050-2Pin_7.0x5.0mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 147.324 82.501 90)
    (descr "SMD Crystal SERIES SMD7050/4 https://www.foxonline.com/pdfs/FQ7050.pdf, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 0.005 180) (layer "F.SilkS") hide)
    (fp_text value "Crystal_Small" (at 0 3.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0 90) (size 3.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(C2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0 90) (size 3.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/crystal.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 168.95 80.9 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "LED_GREEN" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "GPIO25") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.324 92.001)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "QSPI_SS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 169.25 71.825 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.75 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 180) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 54 "D-") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.45 71.587 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VSYS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "USB-C-Connectors-master:TYPE-C-31-M-12" (layer "F.Cu")
    (tedit 6228878E)
    (at 166.5 56.9125 180)
    (descr "Korean Hroparts Elec, Power only USB connector supporting up to 3A")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J7" (at 0 -2.15) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle_USB2.0" (at 0.025 -7.9) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.9 -3.65 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask)
      (solder_mask_margin 0.01) (solder_paste_margin 0.01) (clearance 0.01))
    (pad "" np_thru_hole circle (at -2.9 -3.65 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask)
      (solder_mask_margin 0.01) (solder_paste_margin 0.01) (clearance 0.01))
    (pad "A1" smd rect (at -3.375 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.575 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(J7-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(J7-PadA8)") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 2.575 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.375 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.1 -5.1 180) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.3 -5.1 180) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(J7-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -5.1 180) (size 0.25 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(J7-PadB8)") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" smd rect (at -2.3 -5.1 180) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.1 -5.1 180) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole roundrect (at -4.32 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 67 "unconnected-(J7-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole roundrect (at 4.32 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 67 "unconnected-(J7-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole roundrect (at -4.32 -4.18 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 67 "unconnected-(J7-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole roundrect (at 4.32 -4.18 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 67 "unconnected-(J7-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KIPRJMOD}/USBC.stp"
      (offset (xyz 0 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.074 105.701 -135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 -135) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 -135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 225) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 225) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.824 89.575 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tedit 58641739)
    (at 158 58.4)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "D_Small" (at 0.1 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "VSYS") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "VBUSPIN") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 164.25 68.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "Varistor" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "D+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.424 107.801 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43 45) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 45) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 45) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A429)
    (at 169.725 117.525 -90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at -2.775 -2.025 90) (layer "B.SilkS") hide)
    (fp_text value "Debug" (at 0 -7.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 180) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "SWD") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -5.1 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "Module:Arduino_UNO_R3" locked (layer "B.Cu")
    (tedit 58AB60FC)
    (at 130.87 82.325 -90)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (property "Sheetfile" "File: anac_2040.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at 1.27 3.81 90) (layer "B.SilkS") hide)
    (fp_text value "Arduino_UNO_R3" (at 0 -22.86 90) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+1V1") (pinfunction "X") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3.3V") (pinfunction "IOREF") (pintype "output"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "RST") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3.3V") (pinfunction "3V3") (pintype "power_out"))
    (pad "5" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3.3V") (pinfunction "+5V") (pintype "power_out"))
    (pad "6" thru_hole oval locked (at 12.7 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "GND1") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval locked (at 15.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "GND1") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval locked (at 17.78 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "VSYS") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 22.86 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "GPIO26") (pinfunction "A0") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at 25.4 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GPIO27") (pinfunction "A1") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 27.94 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "GPIO28") (pinfunction "A2") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 30.48 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "GPIO14") (pinfunction "A3") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 33.02 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "GPIO15") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 35.56 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "GPIO16") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (pad "15" thru_hole oval locked (at 35.56 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "GPIO00") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at 33.02 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "GPIO01") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "17" thru_hole oval locked (at 30.48 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GPIO02") (pinfunction "D2") (pintype "bidirectional"))
    (pad "18" thru_hole oval locked (at 27.94 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "GPIO03") (pinfunction "D3") (pintype "bidirectional"))
    (pad "19" thru_hole oval locked (at 25.4 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "GPIO04") (pinfunction "D4") (pintype "bidirectional"))
    (pad "20" thru_hole oval locked (at 22.86 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GPIO05") (pinfunction "D5") (pintype "bidirectional"))
    (pad "21" thru_hole oval locked (at 20.32 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GPIO06") (pinfunction "D6") (pintype "bidirectional"))
    (pad "22" thru_hole oval locked (at 17.78 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "GPIO07") (pinfunction "D7") (pintype "bidirectional"))
    (pad "23" thru_hole oval locked (at 13.72 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "GPIO08") (pinfunction "D8") (pintype "bidirectional"))
    (pad "24" thru_hole oval locked (at 11.18 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "GPIO09") (pinfunction "D9") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 8.64 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "GPIO10") (pinfunction "D10") (pintype "bidirectional"))
    (pad "26" thru_hole oval locked (at 6.1 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "GPIO11") (pinfunction "D11") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 3.56 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "GPIO12") (pinfunction "D12") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at 1.02 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "GPIO13") (pinfunction "D13") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at -1.52 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "GND1") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval locked (at -4.06 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "AREF") (pinfunction "AREF") (pintype "input"))
    (pad "31" thru_hole oval locked (at -6.6 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "GND1") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at -9.14 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "GND1") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_UNO_R3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 163.9 120.45) (end 165.5 120.45) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_circle (center 130.85 68.35) (end 132.45 68.35) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_line (start 181.624 54.701) (end 128.374 54.701) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 135.95 120.45) (end 137.55 120.45) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_circle (center 179.1 69.6) (end 180.7 69.6) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_line (start 131 120.201) (end 133.724 122.951) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 180.124 120.201) (end 181.624 118.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 181.624 118.7) (end 181.624 54.701) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 168.624 120.201) (end 180.124 120.201) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 133.724 122.951) (end 165.924 122.951) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 128.374 120.201) (end 131 120.201) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 165.924 122.951) (end 168.624 120.201) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 128.374 54.701) (end 128.374 120.201) (layer "Edge.Cuts") (width 0.1))
  (gr_text "25" (at 166.85 80.88) (layer "F.SilkS"))
  (gr_text "6" (at 177.174 102.642857) (layer "F.SilkS"))
  (gr_text "22" (at 148.6615 117.551) (layer "F.SilkS"))
  (gr_text "0" (at 177.174 117.9) (layer "F.SilkS"))
  (gr_text "RST" (at 133.693048 87.401) (layer "F.SilkS"))
  (gr_text "25" (at 156.274 117.551) (layer "F.SilkS"))
  (gr_text "19" (at 141.049 117.551) (layer "F.SilkS"))
  (gr_text "Anna2040\nv1,2" (at 168.2 101.7 270) (layer "F.SilkS"))
  (gr_text "3,3v" (at 134.004952 89.951) (layer "F.SilkS"))
  (gr_text "21" (at 146.124 117.551) (layer "F.SilkS"))
  (gr_text "3,3v" (at 134.004952 84.851) (layer "F.SilkS"))
  (gr_text "5" (at 177.174 105.185714) (layer "F.SilkS"))
  (gr_text "12" (at 176.724 85.929) (layer "F.SilkS"))
  (gr_text "4" (at 177.174 107.728571) (layer "F.SilkS"))
  (gr_text "1,1v" (at 134.004952 82.301) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 174.805 113.601 270) (layer "F.SilkS"))
  (gr_text "VIN" (at 133.624 100.151) (layer "F.SilkS"))
  (gr_text "CERN-OHL-P" (at 147.25 120.25) (layer "F.SilkS"))
  (gr_text "11" (at 176.724 88.472) (layer "F.SilkS"))
  (gr_text "27/A1" (at 134.724 107.701) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 169.725 113.743857 270) (layer "F.SilkS"))
  (gr_text "ON" (at 167.024 116.501) (layer "F.SilkS"))
  (gr_text "13" (at 176.724 83.386) (layer "F.SilkS"))
  (gr_text "28/A2" (at 134.724 110.251) (layer "F.SilkS"))
  (gr_text "14" (at 133.295429 112.801) (layer "F.SilkS"))
  (gr_text "3" (at 177.174 110.271428) (layer "F.SilkS"))
  (gr_text "8" (at 177.20019 96.101) (layer "F.SilkS"))
  (gr_text "20" (at 143.5865 117.551) (layer "F.SilkS"))
  (gr_text "+" (at 150.7 56.3) (layer "F.SilkS"))
  (gr_text "AREF" (at 175.866857 78.3) (layer "F.SilkS"))
  (gr_text "9" (at 177.20019 93.558) (layer "F.SilkS"))
  (gr_text "26/A0" (at 134.724 105.151) (layer "F.SilkS"))
  (gr_text "Reset" (at 177.024 66.451) (layer "F.SilkS"))
  (gr_text "18" (at 138.5115 117.551) (layer "F.SilkS"))
  (gr_text "17" (at 135.974 117.551) (layer "F.SilkS"))
  (gr_text "24" (at 153.7365 117.551) (layer "F.SilkS"))
  (gr_text "23" (at 151.199 117.551) (layer "F.SilkS"))
  (gr_text "16" (at 133.295429 117.901) (layer "F.SilkS"))
  (gr_text "7" (at 177.174 100.1) (layer "F.SilkS"))
  (gr_text "2" (at 177.174 112.814285) (layer "F.SilkS"))
  (gr_text "10" (at 176.724 91.015) (layer "F.SilkS"))
  (gr_text "13" (at 173.25 80.88) (layer "F.SilkS"))
  (gr_text "1" (at 177.174 115.357142) (layer "F.SilkS"))
  (gr_text "15" (at 133.274 115.351) (layer "F.SilkS"))
  (gr_text "3,3v" (at 133.974 92.501) (layer "F.SilkS"))
  (gr_text "Boot\nsel." (at 170.024 87.951) (layer "F.SilkS"))
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 154.1 66.6)
        (xy 151.9 66.6)
        (xy 151.9 68.2)
        (xy 151.1 68.2)
        (xy 151.1 72.7)
        (xy 141.9 72.7)
        (xy 141.9 68.7)
        (xy 148.7 68.6)
        (xy 148.7 65.7)
        (xy 154.1 65.7)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (name "3,3v") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 141.951 76.4)
        (xy 141.951 72.7)
        (xy 157.151 72.7)
        (xy 157.151 76.4)
      )
    )
  )
  (zone (net 6) (net_name "VSYS") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 157.3 63.75)
        (xy 151.9 63.75)
        (xy 151.9 65.45)
        (xy 149.9 65.45)
        (xy 149.9 60.05)
        (xy 157.3 60.05)
      )
    )
  )
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 1) (thermal_bridge_width 1) (island_removal_mode 2) (island_area_min 20))
    (polygon
      (pts
        (xy 136.2 73.9)
        (xy 136.2 76.2)
        (xy 134.875 76.2)
        (xy 134.875 73.9)
      )
    )
  )
  (zone (net 5) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 181.3 120)
        (xy 168.4 120)
        (xy 166 122.521926)
        (xy 133.7 122.6)
        (xy 131.2 120)
        (xy 128.52 120)
        (xy 128.52 55.025)
        (xy 181.3 55.025)
      )
    )
  )
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.3 59.8)
        (xy 151.7 59.8)
        (xy 151.7 56.7)
        (xy 154.3 56.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 176.924 87.451)
        (xy 176.574 102.951)
        (xy 174.974 104.151)
        (xy 173.124 104.751)
        (xy 169.374 105.501)
        (xy 165.624 104.551)
        (xy 163.574 103.551)
        (xy 161.674 98.701)
        (xy 161.524 87.401)
      )
    )
  )
)
