(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 415)
    (zones 0)
    (modules 59)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01cc0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad19)")
  (net 2 "Net-(U1-Pad22)")
  (net 3 "Net-(U2-Pad12)")
  (net 4 "Net-(U2-Pad11)")
  (net 5 "Net-(U2-Pad10)")
  (net 6 "Net-(U2-Pad4)")
  (net 7 GND)
  (net 8 "Net-(C1-Pad1)")
  (net 9 VCC)
  (net 10 ~RESET)
  (net 11 DTR)
  (net 12 Batt_Level)
  (net 13 "Net-(C8-Pad2)")
  (net 14 "Net-(C9-Pad2)")
  (net 15 SDA)
  (net 16 SCL)
  (net 17 "Net-(R6-Pad2)")
  (net 18 +BATT)
  (net 19 "Net-(Q1-Pad1)")
  (net 20 D3)
  (net 21 D4)
  (net 22 D5)
  (net 23 D6)
  (net 24 D7)
  (net 25 D8)
  (net 26 D9)
  (net 27 ~SS)
  (net 28 MOSI)
  (net 29 MISO)
  (net 30 SCK)
  (net 31 A1)
  (net 32 A2)
  (net 33 A3)
  (net 34 RxD)
  (net 35 TxD)
  (net 36 D2)
  (net 37 "Net-(J2-Pad1)")
  (net 38 "Net-(U2-Pad13)")
  (net 39 "Net-(D1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net Batt_Level)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net DTR)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad4)")
    (add_net RxD)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net TxD)
    (add_net VCC)
    (add_net ~RESET)
    (add_net ~SS)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142.24 134.62 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5C1823C9)
    (at 133.572 96.510699 180)
    (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U1 (at 0 -5.88) (layer F.SilkS))
    (fp_text value ATmega328P-AU (at 0 5.88) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -4.175 -2.8 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 D3))
    (pad 2 smd roundrect (at -4.175 -2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 D4))
    (pad 3 smd roundrect (at -4.175 -1.2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 4 smd roundrect (at -4.175 -0.4 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 VCC))
    (pad 5 smd roundrect (at -4.175 0.4 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 6 smd roundrect (at -4.175 1.2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 VCC))
    (pad 7 smd roundrect (at -4.175 2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C8-Pad2)"))
    (pad 8 smd roundrect (at -4.175 2.8 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C9-Pad2)"))
    (pad 9 smd roundrect (at -2.8 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 D5))
    (pad 10 smd roundrect (at -2 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 D6))
    (pad 11 smd roundrect (at -1.2 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 D7))
    (pad 12 smd roundrect (at -0.4 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 D8))
    (pad 13 smd roundrect (at 0.4 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 D9))
    (pad 14 smd roundrect (at 1.2 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 ~SS))
    (pad 15 smd roundrect (at 2 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 MOSI))
    (pad 16 smd roundrect (at 2.8 4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 MISO))
    (pad 17 smd roundrect (at 4.175 2.8 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 SCK))
    (pad 18 smd roundrect (at 4.175 2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 VCC))
    (pad 19 smd roundrect (at 4.175 1.2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad19)"))
    (pad 20 smd roundrect (at 4.175 0.4 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C1-Pad1)"))
    (pad 21 smd roundrect (at 4.175 -0.4 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 22 smd roundrect (at 4.175 -1.2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(U1-Pad22)"))
    (pad 23 smd roundrect (at 4.175 -2 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Batt_Level))
    (pad 24 smd roundrect (at 4.175 -2.8 180) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 A1))
    (pad 25 smd roundrect (at 2.8 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 A2))
    (pad 26 smd roundrect (at 2 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 A3))
    (pad 27 smd roundrect (at 1.2 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 SDA))
    (pad 28 smd roundrect (at 0.4 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 SCL))
    (pad 29 smd roundrect (at -0.4 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 ~RESET))
    (pad 30 smd roundrect (at -1.2 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 RxD))
    (pad 31 smd roundrect (at -2 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 TxD))
    (pad 32 smd roundrect (at -2.8 -4.175 180) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 D2))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 132.08 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 129.54 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 127 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 124.46 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 121.92 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 119.38 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.78 134.62 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 147.32 114.3 270)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 157.48 114.3 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x17_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F48A7)
    (at 121.92 116.84 90)
    (descr "Through hole straight pin header, 1x17, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x17 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 0 42.97 90) (layer F.Fab))
    (fp_text user %R (at 0 20.32) (layer F.Fab))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F481D)
    (at 162.56 99.06)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F47F5)
    (at 162.56 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F481A)
    (at 162.56 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4822)
    (at 160.02 99.06)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4816)
    (at 160.02 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F47FC)
    (at 160.02 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4825)
    (at 157.48 99.06)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4812)
    (at 157.48 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4803)
    (at 157.48 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F4808)
    (at 154.94 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F480E)
    (at 154.94 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8F482A)
    (at 154.94 99.06)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
    (fp_text value " " (at 0 2.33) (layer F.Fab))
    (fp_text user " " (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFM:RFM69CW-XXXS2 (layer B.Cu) (tedit 200000)
    (at 133.604 96.52)
    (attr smd)
    (fp_text reference U2 (at -5.82422 9.63422) (layer B.SilkS))
    (fp_text value RFM69CW (at 12.80922 9.63422) (layer B.SilkS))
    (fp_text user 1 (at -4.84886 5.98424) (layer B.SilkS))
    (pad 14 smd rect (at 7.49808 5.99948) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 13 smd rect (at 7.49808 3.99796) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at 7.49808 1.99898) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U2-Pad12)"))
    (pad 11 smd rect (at 7.49808 0) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at 7.49808 -1.99898) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at 7.49808 -3.99796) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 36 D2))
    (pad 8 smd rect (at 7.49808 -5.99948) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 29 MISO))
    (pad 7 smd rect (at -7.49808 -5.99948) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 27 ~SS))
    (pad 6 smd rect (at -7.49808 -3.99796) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 30 SCK))
    (pad 5 smd rect (at -7.49808 -1.99898) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 28 MOSI))
    (pad 4 smd rect (at -7.49808 0) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -7.49808 1.99898) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -7.49808 3.99796) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 1 smd rect (at -7.49808 5.99948) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J2-Pad1)"))
  )
  (module Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering (layer F.Cu) (tedit 5D8CF809)
    (at 161.789 93.939 90)
    (descr LGA-8)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U3 (at 0.015 -2.465 90) (layer F.SilkS))
    (fp_text value BME280 (at 0.015 2.535 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 0.975 -1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 16 SCL))
    (pad 3 smd rect (at 0.325 -1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 15 SDA))
    (pad 2 smd rect (at -0.325 -1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 1 smd rect (at -0.975 -1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 8 smd rect (at -0.975 1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 7 smd rect (at -0.325 1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at 0.325 1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 5 smd rect (at 0.975 1.025 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl
      (offset (xyz 0.01500000025472259 -0.03500000059435272 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 122.936 99.298 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 155.94 90.358)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value PFET (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 122.682 102.87 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value ANT (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 152.334 89.408 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 149.86 99.568 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Batt_Level))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 147.828 99.502 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 470k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Batt_Level))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 161.61 91.186)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 161.61 89.154 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 158.75 90.612 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +BATT))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 145.796 99.552 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Batt_Level))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 148.59 90.408 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 125.746 94.234 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 148.59 95.266 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 157.48 94.168 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 SDA))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 155.194 94.168 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 140.716 96.504 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 125.746 96.266 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 161.56 96.774 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_EuroQuartz_MQ-4pin_7.0x5.0mm (layer F.Cu) (tedit 58CD2E9D)
    (at 144.526 92.964 90)
    (descr "SMD Crystal EuroQuartz MQ series http://cdn-reichelt.de/documents/datenblatt/B400/MQ.pdf, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -3.7 90) (layer F.SilkS))
    (fp_text value 8MHz (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -3.15 -1.25 90) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 3.15 -1.25 90) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 3.15 1.25 90) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -3.15 1.25 90) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_EuroQuartz_MQ-4pin_7.0x5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 145.796 103.14 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 ~RESET))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 DTR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 148.91 102.108 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 ~RESET))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 157.48 86.36 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Batt_in (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +BATT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 147.32 86.36 270)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value EXT_Port1 (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 D5))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D6))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D7))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D8))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 MOSI))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 MISO))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SCK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8CFEF0)
    (at 152.4 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Analog2 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 31 A1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8CFEE9)
    (at 152.4 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value ProtoVCC (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5D8CFEE1)
    (at 152.4 99.06)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value ProtoGND (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.4 94.11 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -2.28 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 VCC))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 122.936 91.6155 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 22k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 VCC))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 ~SS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 152 86 270)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value Rot (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 134.112 89.662 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 D9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.78 106.68 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value ArduProg (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 RxD))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 TxD))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 DTR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.4455 103.378 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 A1))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142.24 106.68 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value EXT_Port2 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D4))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 SCL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 SDA))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 A3))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 A2))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 ~RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RFM69CW (at 134.112 88.646) (layer Eco2.User))
  (gr_text 1 (at 125.984 104.14) (layer Eco2.User))
  (gr_text 1 (at 147.32 97.028) (layer Eco1.User))
  (gr_text 1 (at 137.668 100.584) (layer Eco1.User))
  (gr_line (start 120.65 111.76) (end 120.65 137.16) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 154.305 110.49) (end 155.305 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 131.445 110.49) (end 132.445 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_text ANT (at 123.698 104.14 90) (layer Eco1.User))
  (gr_text "MSN R00 (SE 2019)" (at 121.666 94.996 90) (layer F.Cu))
  (gr_text "A1  VCC  GND" (at 151.13 101.6 90) (layer Eco1.User))
  (gr_text "RST   A2   A3   SDA  SCL  D3   D4   GND GND  VCC  RxD  TxD  DTR" (at 142.24 108.204) (layer Eco1.User))
  (gr_text "GND  BATT" (at 156.21 84.836) (layer Eco1.User))
  (gr_text "SCK MISO MOSI  D8   D7   D6   D5  GND  VCC\n" (at 137.16 84.836) (layer Eco1.User))
  (gr_line (start 152.4 109.22) (end 152.4 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 133.35 109.22) (end 133.35 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 129.54 109.22) (end 129.54 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 156.21 109.22) (end 156.21 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 133.35 109.22) (end 152.4 109.22) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 133.35 111.76) (end 152.4 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 156.21 111.76) (end 164.465 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 156.21 109.22) (end 164.465 109.22) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 164.465 137.16) (end 164.465 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 129.54 111.76) (end 120.65 111.76) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 120.65 137.16) (end 164.465 137.16) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 120.65 109.22) (end 129.54 109.22) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 164.465 109.22) (end 164.465 83.82) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 120.65 83.82) (end 120.65 109.22) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 164.465 83.82) (end 120.65 83.82) (layer Edge.Cuts) (width 0.12))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.904 84.074) (xy 164.084 84.074) (xy 164.084 108.966) (xy 120.904 108.966)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.904 84.074) (xy 164.084 84.074) (xy 164.084 108.966) (xy 120.904 108.966)
      )
    )
  )
)
