<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<library>
<description>Generated from &lt;b&gt;luftdaten_v1r1.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="LOLIN_LOLINV3">
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-02-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-02-PACKAGE-ROUND-PAD">
<description>&lt;b&gt;JST XH Connector Round Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-03-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;3&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-03-PACKAGE-ROUND-PAD">
<description>&lt;b&gt;JST XH Connector Round Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;3&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-04-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;
Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;4&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-04-PACKAGE-ROUND-PAD">
<description>&lt;b&gt;JST XH Connector Round Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;4&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-05-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;5&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-05-PACKAGE-ROUND-PAD">
<description>&lt;b&gt;JST XH Connector Round Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;5&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="BB2359_BB2359">
</package>
<package name="DCDC-POWERMODULES_SG053-SZ">
</package>
<package name="HEADER-1P27-PERSO_FE08-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="JUMPER_SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="JUMPER_SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="LED_1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="LED_CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="LED_CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="LED_CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="LED_CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="LED_CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="LED_CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="LED_IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="LED_KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
<package name="LED_LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LED_LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="LED_LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED_LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED_LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="LED_LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LED_LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LED_LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LED_LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="LED_MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="LED_MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="LED_OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="LED_OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="LED_P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="LED_P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="LED_P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="LED_Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LED_Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LED_Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LED_Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LED_SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="LED_SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="LED_SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="LED_SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="LED_SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
<package name="LED_SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="LED_SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
<package name="LED_U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="PMS7003_PMS7003">
</package>
<package name="RCL_0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="RCL_0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="RCL_0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="RCL_0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="RCL_0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="RCL_0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="RCL_0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="RCL_0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="RCL_0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="RCL_0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="RCL_0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="RCL_0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="RCL_0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="RCL_0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="RCL_0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="RCL_0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="RCL_0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="RCL_0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="RCL_0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="RCL_0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="RCL_0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="RCL_0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="RCL_1812X7R">
<description>&lt;b&gt;Chip Monolithic Ceramic Capacitors&lt;/b&gt; Medium Voltage High Capacitance for General Use&lt;p&gt;
Source: http://www.murata.com .. GRM43DR72E224KW01.pdf</description>
</package>
<package name="RCL_M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="RCL_M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="RCL_M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="RCL_M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="RCL_M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="RCL_MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="RCL_P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="RCL_P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="RCL_P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="RCL_PRL1632">
<description>&lt;b&gt;PRL1632 are realized as 1W for 3.2 × 1.6mm(1206)&lt;/b&gt;&lt;p&gt;
Source: http://www.mouser.com/ds/2/392/products_18-2245.pdf</description>
</package>
<package name="RCL_R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="RCL_R0402">
<description>&lt;b&gt;Chip RESISTOR 0402 EIA (1005 Metric)&lt;/b&gt;</description>
</package>
<package name="RCL_R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL_R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;</description>
</package>
<package name="RCL_R01005">
</package>
<package name="RCL_R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R1218">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
</package>
<package name="RCL_R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R4527">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
</package>
<package name="RCL_R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="RCL_R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="RCL_RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="RCL_V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="RCL_V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="RCL_V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="RCL_VMTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VMTB60">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC60&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA52">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR52&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA53">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR53&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA54">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR54&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA56">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR56&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_WSC0001">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC01/2">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC0002">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC2515">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC4527">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC6927">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL-PERSO_085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RCL-PERSO_A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 reflow solder&lt;/b&gt;&lt;p&gt;KEMET S / EIA 3216-12</description>
</package>
<package name="RCL-PERSO_A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="RCL-PERSO_B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 reflow solder&lt;/b&gt;&lt;p&gt;KEMET T / EIA 3528-12</description>
</package>
<package name="RCL-PERSO_B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="RCL-PERSO_B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="RCL-PERSO_B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="RCL-PERSO_C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 reflow solder&lt;/b&gt;&lt;p&gt;KEMET U / EIA 6032-15</description>
</package>
<package name="RCL-PERSO_C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="RCL-PERSO_CT3216">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_CT3528">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_CT6032">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 reflow solder</description>
</package>
<package name="RCL-PERSO_D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="RCL-PERSO_E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 reflow solder&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="RCL-PERSO_E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="RCL-PERSO_E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="RCL-PERSO_E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="RCL-PERSO_E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="RCL-PERSO_E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="RCL-PERSO_E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="RCL-PERSO_E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="RCL-PERSO_E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="RCL-PERSO_E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="RCL-PERSO_E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="RCL-PERSO_E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="RCL-PERSO_E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="RCL-PERSO_E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="RCL-PERSO_E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="RCL-PERSO_E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="RCL-PERSO_E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="RCL-PERSO_E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="RCL-PERSO_E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="RCL-PERSO_E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="RCL-PERSO_E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="RCL-PERSO_E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="RCL-PERSO_E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="RCL-PERSO_E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="RCL-PERSO_E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="RCL-PERSO_E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="RCL-PERSO_E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="RCL-PERSO_E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="RCL-PERSO_E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="RCL-PERSO_E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="RCL-PERSO_E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="RCL-PERSO_E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="RCL-PERSO_E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="RCL-PERSO_E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="RCL-PERSO_E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="RCL-PERSO_E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="RCL-PERSO_E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="RCL-PERSO_E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="RCL-PERSO_E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="RCL-PERSO_E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="RCL-PERSO_E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="RCL-PERSO_E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="RCL-PERSO_E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="RCL-PERSO_E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="RCL-PERSO_EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="RCL-PERSO_EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="RCL-PERSO_EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="RCL-PERSO_EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="RCL-PERSO_EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="RCL-PERSO_ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="RCL-PERSO_ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="RCL-PERSO_P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL-PERSO_P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL-PERSO_P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL-PERSO_P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 reflow solder&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_9E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_9F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_A">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_A'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_B">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_B'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_C">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_C'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_D">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E1">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E9">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_E13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_F'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_F0">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_F13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_G">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_H">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_A5">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_B6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SANYO-OSCON_SMD_F12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="RCL-PERSO_SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_P">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_SMC_Z">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="RCL-PERSO_TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="RCL-PERSO_TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="RCL-PERSO_UD-4X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 4 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="RCL-PERSO_UD-5X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 5 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="RCL-PERSO_UD-6,3X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="RCL-PERSO_UD-6,3X7,7_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 7.7 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="RCL-PERSO_UD-8X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 8 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="RCL-PERSO_UD-10X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 10 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="SDS011_SDS011">
</package>
</packages>
<symbols>
<symbol name="LOLIN_LOLIL">
<pin name="3V"/>
<pin name="3V1"/>
<pin name="3V3"/>
<pin name="A0"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="RST"/>
<pin name="RX"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="SC"/>
<pin name="SK"/>
<pin name="SO"/>
<pin name="TX"/>
<pin name="VIN"/>
<pin name="VV"/>
</symbol>
<symbol name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BB2359_BB2359">
<pin name="DS" direction="in"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="VOUT"/>
</symbol>
<symbol name="DCDC-POWERMODULES_SG053-SZ">
<pin name="+IN"/>
<pin name="+OUT"/>
<pin name="-IN"/>
<pin name="-OUT"/>
</symbol>
<symbol name="FRAMES_A4L-LOC">
</symbol>
<symbol name="HEADER-1P27-PERSO_FE08-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="JUMPER_SJ">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LED_LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PMS7003_PMS7003">
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="RESET"/>
<pin name="RX" direction="in"/>
<pin name="SET"/>
<pin name="TX" direction="out"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
</symbol>
<symbol name="RCL_R-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RCL-PERSO_CPOL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SDS011_SDS011">
</symbol>
<symbol name="SUPPLY1_+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="SUPPLY1_+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="SUPPLY2_GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SUPPLY2_V+">
<pin name="V+" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LOLIN_LOLINV3" prefix="IC" uservalue="yes">
<gates>
<gate name="NODEMCU-LOLINV.3" symbol="LOLIN_LOLIL"/>
</gates>
<devices>
<device name="" package="LOLIN_LOLINV3">
<connects>
<connect gate="NODEMCU-LOLINV.3" pin="3V" pad="3"/>
<connect gate="NODEMCU-LOLINV.3" pin="3V1" pad="3V"/>
<connect gate="NODEMCU-LOLINV.3" pin="3V3" pad="3V1 3V3"/>
<connect gate="NODEMCU-LOLINV.3" pin="A0" pad="A0 A1"/>
<connect gate="NODEMCU-LOLINV.3" pin="D0" pad="D0"/>
<connect gate="NODEMCU-LOLINV.3" pin="D1" pad="D1"/>
<connect gate="NODEMCU-LOLINV.3" pin="D2" pad="D2"/>
<connect gate="NODEMCU-LOLINV.3" pin="D3" pad="D3"/>
<connect gate="NODEMCU-LOLINV.3" pin="D4" pad="D4"/>
<connect gate="NODEMCU-LOLINV.3" pin="D5" pad="D5"/>
<connect gate="NODEMCU-LOLINV.3" pin="D6" pad="D6"/>
<connect gate="NODEMCU-LOLINV.3" pin="D7" pad="D7"/>
<connect gate="NODEMCU-LOLINV.3" pin="D8" pad="D8"/>
<connect gate="NODEMCU-LOLINV.3" pin="EN" pad="EN EN1"/>
<connect gate="NODEMCU-LOLINV.3" pin="GND" pad="GND"/>
<connect gate="NODEMCU-LOLINV.3" pin="GND1" pad="GND1"/>
<connect gate="NODEMCU-LOLINV.3" pin="GND2" pad="GND2 GND5"/>
<connect gate="NODEMCU-LOLINV.3" pin="GND3" pad="GND3 GND6"/>
<connect gate="NODEMCU-LOLINV.3" pin="GND4" pad="GND4 GND7"/>
<connect gate="NODEMCU-LOLINV.3" pin="RST" pad="RST RST1"/>
<connect gate="NODEMCU-LOLINV.3" pin="RX" pad="RX"/>
<connect gate="NODEMCU-LOLINV.3" pin="S1" pad="S1 S4"/>
<connect gate="NODEMCU-LOLINV.3" pin="S2" pad="S2 S5"/>
<connect gate="NODEMCU-LOLINV.3" pin="S3" pad="S3 S6"/>
<connect gate="NODEMCU-LOLINV.3" pin="SC" pad="SC SC1"/>
<connect gate="NODEMCU-LOLINV.3" pin="SK" pad="SK SK1"/>
<connect gate="NODEMCU-LOLINV.3" pin="SO" pad="SO SO1"/>
<connect gate="NODEMCU-LOLINV.3" pin="TX" pad="TX"/>
<connect gate="NODEMCU-LOLINV.3" pin="VIN" pad="VIN VIN1"/>
<connect gate="NODEMCU-LOLINV.3" pin="VV" pad="VV VV1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-02-PIN" prefix="X">
<description>&lt;b&gt;JST XH Connector 2 Pin&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="-1" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_MV"/>
<gate name="-2" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
</gates>
<devices>
<device name="-LONG-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-02-PACKAGE-LONG-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ROUND-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-02-PACKAGE-ROUND-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-03-PIN" prefix="X">
<description>&lt;b&gt;JST XH Connector 2 Pin&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;3&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="-1" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_MV"/>
<gate name="-2" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-3" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
</gates>
<devices>
<device name="-LONG-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-03-PACKAGE-LONG-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ROUND-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-03-PACKAGE-ROUND-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-04-PIN" prefix="X">
<description>&lt;b&gt;JST XH Connector 2 Pin&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;4&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="-1" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_MV"/>
<gate name="-2" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-3" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-4" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
</gates>
<devices>
<device name="-LONG-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-04-PACKAGE-LONG-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ROUND-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-04-PACKAGE-ROUND-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-05-PIN" prefix="X">
<description>&lt;b&gt;JST XH Connector 2 Pin&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;5&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="-1" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_MV"/>
<gate name="-2" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-3" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-4" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
<gate name="-5" symbol="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_M"/>
</gates>
<devices>
<device name="-LONG-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-05-PACKAGE-LONG-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ROUND-PAD" package="REMBRANDT-ELECTRONICS---JST-XH-CONNECTORS-V1-0_JST-XH-05-PACKAGE-ROUND-PAD">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB2359_BB2359">
<gates>
<gate name="G$1" symbol="BB2359_BB2359"/>
</gates>
<devices>
<device name="" package="BB2359_BB2359">
<connects>
<connect gate="G$1" pin="DS" pad="P1"/>
<connect gate="G$1" pin="GND" pad="P3"/>
<connect gate="G$1" pin="VIN" pad="P2"/>
<connect gate="G$1" pin="VOUT" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCDC-POWERMODULES_SG053-SZ">
<gates>
<gate name="G$1" symbol="DCDC-POWERMODULES_SG053-SZ"/>
</gates>
<devices>
<device name="" package="DCDC-POWERMODULES_SG053-SZ">
<connects>
<connect gate="G$1" pin="+IN" pad="P$3 P$4"/>
<connect gate="G$1" pin="+OUT" pad="P$5 P$6"/>
<connect gate="G$1" pin="-IN" pad="P$1 P$2"/>
<connect gate="G$1" pin="-OUT" pad="P$7 P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAMES_A4L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="FRAMES_A4L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1P27-PERSO_FE08-2" prefix="SV" uservalue="yes">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="HEADER-1P27-PERSO_FE08-2"/>
</gates>
<devices>
<device name="" package="HEADER-1P27-PERSO_FE08-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER_SJ" prefix="SJ" uservalue="yes">
<description>SMD solder &lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="JUMPER_SJ"/>
</gates>
<devices>
<device name="" package="JUMPER_SJ">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="JUMPER_SJW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED_LED"/>
</gates>
<devices>
<device name="" package="LED_SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LED_LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LED_LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED_LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED_LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED_LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="LED_Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="LED_Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="LED_Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="LED_Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="LED_CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="LED_CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="LED_CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="LED_CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="LED_CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="LED_CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="LED_IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KA-3528ASYC" package="LED_KA-3528ASYC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LED_LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LED_LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LED_LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="LED_MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="LED_OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="LED_P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="LED_P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="LED_P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="LED_SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="LED_SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="LED_OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="LED_SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0603" package="LED_SML0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0805" package="LED_SML0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML1206" package="LED_SML1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT1206" package="LED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED_LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="LED_U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="LED_MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMS7003_PMS7003">
<gates>
<gate name="G$1" symbol="PMS7003_PMS7003"/>
</gates>
<devices>
<device name="" package="PMS7003_PMS7003">
<connects>
<connect gate="G$1" pin="GND1" pad="Q3"/>
<connect gate="G$1" pin="GND2" pad="Q4"/>
<connect gate="G$1" pin="RESET" pad="Q5"/>
<connect gate="G$1" pin="RX" pad="Q7"/>
<connect gate="G$1" pin="SET" pad="Q10"/>
<connect gate="G$1" pin="TX" pad="Q9"/>
<connect gate="G$1" pin="VCC1" pad="Q1"/>
<connect gate="G$1" pin="VCC2" pad="Q2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCL_R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="RCL_R-EU"/>
</gates>
<devices>
<device name="0204/2V" package="RCL_0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0204/5" package="RCL_0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0204/7" package="RCL_0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/2V" package="RCL_0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/5V" package="RCL_0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/7" package="RCL_0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/10" package="RCL_0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/12" package="RCL_0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0207/15" package="RCL_0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0309/10" package="RCL_0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0309/12" package="RCL_0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0309/V" package="RCL_0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0411/3V" package="RCL_0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0411/12" package="RCL_0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0411/15" package="RCL_0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0414/5V" package="RCL_0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0414/15" package="RCL_0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0613/5V" package="RCL_P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0613/15" package="RCL_P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0617/5V" package="RCL_0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0617/17" package="RCL_0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0617/22" package="RCL_0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0817/7V" package="RCL_P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0817/22" package="RCL_P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0922/22" package="RCL_0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="0922V" package="RCL_0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="01005" package="RCL_R01005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="1812X7R" package="RCL_1812X7R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M0805" package="RCL_M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M1206" package="RCL_M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M1406" package="RCL_M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M2012" package="RCL_M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M2309" package="RCL_M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M3216" package="RCL_M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M3516" package="RCL_M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="M5923" package="RCL_M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0102AX" package="RCL_MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0102R" package="RCL_MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0102W" package="RCL_MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0204R" package="RCL_MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0204W" package="RCL_MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0207R" package="RCL_MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="MELF0207W" package="RCL_MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="PRL1632" package="RCL_PRL1632">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R0201" package="RCL_R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R0402" package="RCL_R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R0603" package="RCL_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R0805" package="RCL_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R0805W" package="RCL_R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R1206" package="RCL_R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R1206W" package="RCL_R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R1210" package="RCL_R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R1210W" package="RCL_R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R1218" package="RCL_R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2010" package="RCL_R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2010W" package="RCL_R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2012" package="RCL_R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2012W" package="RCL_R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2512" package="RCL_R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R2512W" package="RCL_R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R3216" package="RCL_R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R3216W" package="RCL_R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R3225" package="RCL_R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R3225W" package="RCL_R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R4527" package="RCL_R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R5025" package="RCL_R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R5025W" package="RCL_R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R6332" package="RCL_R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="R6332W" package="RCL_R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="RDH/15" package="RCL_RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="V234/12" package="RCL_V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="V235/17" package="RCL_V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="V526-0" package="RCL_V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VMTA55" package="RCL_VMTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VMTB60" package="RCL_VMTB60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VTA52" package="RCL_VTA52">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VTA53" package="RCL_VTA53">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VTA54" package="RCL_VTA54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VTA55" package="RCL_VTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="VTA56" package="RCL_VTA56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC0001" package="RCL_WSC0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC01/2" package="RCL_WSC01/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC0002" package="RCL_WSC0002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC2515" package="RCL_WSC2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC4527" package="RCL_WSC4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
<device name="WSC6927" package="RCL_WSC6927">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCL-PERSO_CPOL-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="RCL-PERSO_CPOL"/>
</gates>
<devices>
<device name="085CS-1AR" package="RCL-PERSO_085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1AW" package="RCL-PERSO_085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1R" package="RCL-PERSO_085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1W" package="RCL-PERSO_085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-2R" package="RCL-PERSO_139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-2W" package="RCL-PERSO_139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-3R" package="RCL-PERSO_139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-3W" package="RCL-PERSO_139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-0810" package="RCL-PERSO_140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-1010" package="RCL-PERSO_140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-1014" package="RCL-PERSO_140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-0810" package="RCL-PERSO_150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-1010" package="RCL-PERSO_150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-1014" package="RCL-PERSO_150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0405" package="RCL-PERSO_153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0505" package="RCL-PERSO_153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0605" package="RCL-PERSO_153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0807" package="RCL-PERSO_153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0810" package="RCL-PERSO_153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1010" package="RCL-PERSO_153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1012" package="RCL-PERSO_153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1014" package="RCL-PERSO_153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="175TMP-0808" package="RCL-PERSO_175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="175TMP-0810" package="RCL-PERSO_175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A" package="RCL-PERSO_PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A/3216-18R" package="RCL-PERSO_A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A/3216-18W" package="RCL-PERSO_A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B" package="RCL-PERSO_PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B/3528-21R" package="RCL-PERSO_B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B/3528-21W" package="RCL-PERSO_B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181A" package="RCL-PERSO_B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181B" package="RCL-PERSO_B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181C" package="RCL-PERSO_B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181D" package="RCL-PERSO_B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C" package="RCL-PERSO_PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C/6032-28R" package="RCL-PERSO_C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C/6032-28W" package="RCL-PERSO_C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT3216" package="RCL-PERSO_CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT3528" package="RCL-PERSO_CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT6032" package="RCL-PERSO_CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT7343" package="RCL-PERSO_CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D" package="RCL-PERSO_PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D/7343-31R" package="RCL-PERSO_D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D/7343-31W" package="RCL-PERSO_D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E" package="RCL-PERSO_PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E/7260-38R" package="RCL-PERSO_E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E/7260-38W" package="RCL-PERSO_E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E1.8-4" package="RCL-PERSO_E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2,5-6E" package="RCL-PERSO_E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2-4" package="RCL-PERSO_E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2-5" package="RCL-PERSO_E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-4V" package="RCL-PERSO_E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-5" package="RCL-PERSO_E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-5V" package="RCL-PERSO_E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-6" package="RCL-PERSO_E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-7" package="RCL-PERSO_E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E3.5-8" package="RCL-PERSO_E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E3.5-10" package="RCL-PERSO_E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-4" package="RCL-PERSO_E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-5" package="RCL-PERSO_E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-6" package="RCL-PERSO_E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-8.5" package="RCL-PERSO_E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-9VAXIAL" package="RCL-PERSO_E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-10.5" package="RCL-PERSO_E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-13" package="RCL-PERSO_E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E7.5-16" package="RCL-PERSO_E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E7.5-18" package="RCL-PERSO_E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-20" package="RCL-PERSO_EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-22.5" package="RCL-PERSO_EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-25" package="RCL-PERSO_EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-30" package="RCL-PERSO_EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-35" package="RCL-PERSO_EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-5AXIAL" package="RCL-PERSO_E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-6AXIAL" package="RCL-PERSO_E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-9AXIAL" package="RCL-PERSO_E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-6AXIAL" package="RCL-PERSO_E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-9AXIAL" package="RCL-PERSO_E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-10AXIAL" package="RCL-PERSO_E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E25-9AXIAL" package="RCL-PERSO_E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E25-10AXIAL" package="RCL-PERSO_E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-10AXIAL" package="RCL-PERSO_E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-12AXIAL" package="RCL-PERSO_E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-16AXIAL" package="RCL-PERSO_E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-12AXIAL" package="RCL-PERSO_E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-14AXIAL" package="RCL-PERSO_E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-16AXIAL" package="RCL-PERSO_E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-18AXIAL" package="RCL-PERSO_E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-16AXIAL" package="RCL-PERSO_E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-18AXIAL" package="RCL-PERSO_E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-21AXIAL" package="RCL-PERSO_E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-22AXIAL" package="RCL-PERSO_E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-25AXIAL" package="RCL-PERSO_E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E50-25AXIAL" package="RCL-PERSO_E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E50-30AXIAL" package="RCL-PERSO_E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E55-25AXIAL" package="RCL-PERSO_E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E55-30AXIAL" package="RCL-PERSO_E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR1" package="RCL-PERSO_ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR2" package="RCL-PERSO_ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR3" package="RCL-PERSO_ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR4" package="RCL-PERSO_ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR5" package="RCL-PERSO_ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="F" package="RCL-PERSO_PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="G" package="RCL-PERSO_PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-35" package="RCL-PERSO_P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-40" package="RCL-PERSO_P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-50" package="RCL-PERSO_P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-60" package="RCL-PERSO_P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="R/2012-12R" package="RCL-PERSO_R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="R/2012-12W" package="RCL-PERSO_R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_9E" package="RCL-PERSO_SANYO-OSCON_9E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_9F" package="RCL-PERSO_SANYO-OSCON_9F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_A" package="RCL-PERSO_SANYO-OSCON_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_A'" package="RCL-PERSO_SANYO-OSCON_A'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_B" package="RCL-PERSO_SANYO-OSCON_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_B'" package="RCL-PERSO_SANYO-OSCON_B'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C" package="RCL-PERSO_SANYO-OSCON_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C'" package="RCL-PERSO_SANYO-OSCON_C'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C6" package="RCL-PERSO_SANYO-OSCON_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_D" package="RCL-PERSO_SANYO-OSCON_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E" package="RCL-PERSO_SANYO-OSCON_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E'" package="RCL-PERSO_SANYO-OSCON_E'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E1" package="RCL-PERSO_SANYO-OSCON_E1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E7" package="RCL-PERSO_SANYO-OSCON_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E9" package="RCL-PERSO_SANYO-OSCON_E9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E12" package="RCL-PERSO_SANYO-OSCON_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E13" package="RCL-PERSO_SANYO-OSCON_E13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F" package="RCL-PERSO_SANYO-OSCON_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F'" package="RCL-PERSO_SANYO-OSCON_F'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F0" package="RCL-PERSO_SANYO-OSCON_F0">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F8" package="RCL-PERSO_SANYO-OSCON_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F13" package="RCL-PERSO_SANYO-OSCON_F13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_G" package="RCL-PERSO_SANYO-OSCON_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_H" package="RCL-PERSO_SANYO-OSCON_H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_A5" package="RCL-PERSO_SANYO-OSCON_SMD_A5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_B6" package="RCL-PERSO_SANYO-OSCON_SMD_B6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_C6" package="RCL-PERSO_SANYO-OSCON_SMD_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_E7" package="RCL-PERSO_SANYO-OSCON_SMD_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_E12" package="RCL-PERSO_SANYO-OSCON_SMD_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_F8" package="RCL-PERSO_SANYO-OSCON_SMD_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_F12" package="RCL-PERSO_SANYO-OSCON_SMD_F12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCA" package="RCL-PERSO_SMC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCB" package="RCL-PERSO_SMC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCC" package="RCL-PERSO_SMC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCD" package="RCL-PERSO_SMC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCE" package="RCL-PERSO_SMC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCP" package="RCL-PERSO_SMC_P">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCZ" package="RCL-PERSO_SMC_Z">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-45" package="RCL-PERSO_TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-50" package="RCL-PERSO_TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-60" package="RCL-PERSO_TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-70" package="RCL-PERSO_TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-80" package="RCL-PERSO_TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D4" package="RCL-PERSO_TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D4L" package="RCL-PERSO_TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D5" package="RCL-PERSO_TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D5L" package="RCL-PERSO_TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D6" package="RCL-PERSO_TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D6L" package="RCL-PERSO_TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D7" package="RCL-PERSO_TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D7L" package="RCL-PERSO_TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D6L" package="RCL-PERSO_TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D7" package="RCL-PERSO_TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D7L" package="RCL-PERSO_TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D9" package="RCL-PERSO_TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D9L" package="RCL-PERSO_TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D10" package="RCL-PERSO_TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D11" package="RCL-PERSO_TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D11L" package="RCL-PERSO_TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT6D6" package="RCL-PERSO_TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-4X5,8" package="RCL-PERSO_UD-4X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-5X5,8" package="RCL-PERSO_UD-5X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-6,3X7,7" package="RCL-PERSO_UD-6,3X7,7_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-6,3X8,8" package="RCL-PERSO_UD-6,3X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-8X10" package="RCL-PERSO_UD-8X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-10X10" package="RCL-PERSO_UD-10X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDS011_SDSO11">
<gates>
<gate name="G$1" symbol="SDS011_SDS011"/>
</gates>
<devices>
<device name="" package="SDS011_SDS011">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY1_+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SUPPLY1_+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY1_+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SUPPLY1_+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY2_GND" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="GND" symbol="SUPPLY2_GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY2_V+" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SUPPLY2_V+"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
