(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.64)
  )
  (paper "A4")
  (title_block
    (title "ESP32s3APRS by F4JMZ")
    (date "2024-08-24")
    (rev "0.0.1")
    (company "©️2025 Marc CAPDEVILLE (F4JMZ)")
    (comment 1 "Sources : https://github.com/mcapdeville/esp32s3aprs")
    (comment 2 "Licensed under CERN-OHL-S v2 (https://ohwr.org/cern_ohl_s_v2.txt)")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.55) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance_ratio -0.05)
    (grid_origin 100 50)
    (pcbplotparams
      (layerselection 0x00312fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab true)
      (subtractmaskfromsilk true)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "ESP32_APRS-ddf/")
    )
  )
  (property "Copyright" "©️2025 Marc CAPDEVILLE (F4JMZ)")
  (property "License" "Licensed under CERN-OHL-S v2 or any later version")
  (property "Source" "https://github.com/mcapdeville/esp32s3aprs")
  (net 0 "")
  (net 1 "GND")
  (net 2 "VBUS")
  (net 3 "+BATT")
  (net 4 "+3V3")
  (net 5 "Net-(C203-Pad1)")
  (net 6 "Net-(C204-Pad2)")
  (net 7 "Net-(C204-Pad1)")
  (net 8 "Net-(C205-Pad1)")
  (net 9 "Net-(C207-Pad1)")
  (net 10 "Net-(C301-Pad1)")
  (net 11 "Net-(C110-Pad1)")
  (net 12 "Net-(C404-Pad1)")
  (net 13 "Net-(C501-Pad1)")
  (net 14 "Net-(C503-Pad1)")
  (net 15 "Net-(D203-Pad1)")
  (net 16 "Net-(J202-PadB5)")
  (net 17 "Net-(J202-PadA5)")
  (net 18 "/SA8x8/SATX")
  (net 19 "/SA8x8/SAAUDIO_ON")
  (net 20 "Net-(Q201-Pad1)")
  (net 21 "/SA8x8/SARX")
  (net 22 "Net-(J301-Pad1)")
  (net 23 "Net-(C101-Pad1)")
  (net 24 "Net-(C303-Pad1)")
  (net 25 "/SA8x8/In")
  (net 26 "/SA8x8/Out")
  (net 27 "Net-(C411-Pad2)")
  (net 28 "Net-(J501-Pad2)")
  (net 29 "Net-(Q403-Pad3)")
  (net 30 "Net-(Q403-Pad1)")
  (net 31 "Net-(Q406-Pad1)")
  (net 32 "/SA8x8/SAHL")
  (net 33 "/SA8x8/SAPD")
  (net 34 "/SA8x8/SAPTT")
  (net 35 "/SQ")
  (net 36 "/U2RX")
  (net 37 "/U2TX")
  (net 38 "/AudioIn")
  (net 39 "Net-(C401-Pad1)")
  (net 40 "/Ptt")
  (net 41 "/HL")
  (net 42 "/BUSY")
  (net 43 "/GPSRESET")
  (net 44 "/U1TX")
  (net 45 "/PD")
  (net 46 "/USB Charger/INOKB")
  (net 47 "/USB Charger/Stat")
  (net 48 "/USB Charger/CHGOFF")
  (net 49 "/USB Charger/ENBST")
  (net 50 "/ESP32-S3-WROOM/GPIO18")
  (net 51 "/ESP32-S3-WROOM/GPIO17")
  (net 52 "/ESP32-S3-WROOM/GPIO16")
  (net 53 "/ESP32-S3-WROOM/GPIO15")
  (net 54 "/ESP32-S3-WROOM/GPIO7")
  (net 55 "/ESP32-S3-WROOM/GPIO6")
  (net 56 "/ESP32-S3-WROOM/GPIO5")
  (net 57 "/ESP32-S3-WROOM/GPIO4")
  (net 58 "Net-(R203-Pad1)")
  (net 59 "/ESP32-S3-WROOM/D-")
  (net 60 "/ESP32-S3-WROOM/D+")
  (net 61 "Net-(C201-Pad1)")
  (net 62 "Net-(C401-Pad2)")
  (net 63 "Net-(C601-Pad1)")
  (net 64 "Net-(C606-Pad1)")
  (net 65 "Net-(C607-Pad1)")
  (net 66 "Net-(C608-Pad1)")
  (net 67 "Net-(C609-Pad1)")
  (net 68 "Net-(C610-Pad1)")
  (net 69 "Net-(C611-Pad2)")
  (net 70 "Net-(C611-Pad1)")
  (net 71 "/FORCE_ON")
  (net 72 "/FSPID")
  (net 73 "/FSSPICLK")
  (net 74 "Net-(J601-Pad8)")
  (net 75 "Net-(J601-Pad3)")
  (net 76 "Net-(J601-Pad2)")
  (net 77 "Net-(Q101-Pad3)")
  (net 78 "Net-(Q101-Pad1)")
  (net 79 "Net-(Q102-Pad3)")
  (net 80 "Net-(Q102-Pad1)")
  (net 81 "/BAT_ADC")
  (net 82 "/SW3")
  (net 83 "/SW2")
  (net 84 "/SW1")
  (net 85 "Net-(D301-Pad1)")
  (net 86 "Net-(D402-Pad3)")
  (net 87 "Net-(R414-Pad2)")
  (net 88 "/USB Charger/Vsys")
  (net 89 "/ESP32-S3-WROOM/Boot")
  (net 90 "Net-(Q501-Pad1)")
  (net 91 "/USB Charger/D+")
  (net 92 "/USB Charger/D-")
  (net 93 "/USB Charger/USB_P")
  (net 94 "/USB Charger/USB_N")
  (net 95 "/FSPICS0")
  (net 96 "/DC")
  (net 97 "/GPS1PPS")
  (net 98 "/U1RX")
  (net 99 "Net-(C106-Pad1)")
  (net 100 "/E-paper display/PON")
  (net 101 "/E-paper display/CS")
  (net 102 "/L86-M33/GPS1PPS")
  (net 103 "/E-paper display/SCLK")
  (net 104 "/E-paper display/SDAT")
  (net 105 "/L86-M33/GPSRESET")
  (net 106 "/L86-M33/GPSAADET_N")
  (net 107 "/L86-M33/GPSRX")
  (net 108 "/L86-M33/GPSTX")
  (net 109 "/ESP32-S3-WROOM/GPIO0")
  (net 110 "/ESP32-S3-WROOM/GPIO1")
  (net 111 "Net-(J501-Pad3)")
  (net 112 "Net-(C408-Pad1)")
  (net 113 "Net-(C504-Pad2)")
  (net 114 "Net-(C505-Pad2)")
  (net 115 "Net-(C506-Pad2)")
  (net 116 "Net-(C507-Pad2)")
  (net 117 "Net-(J105-Pad2)")
  (net 118 "Net-(J106-Pad8)")
  (net 119 "Net-(J108-Pad1)")
  (net 120 "Net-(J602-Pad1)")
  (net 121 "Net-(J204-Pad1)")
  (net 122 "unconnected-(J202-PadA8)")
  (net 123 "unconnected-(J202-PadB8)")
  (net 124 "unconnected-(J601-Pad1)")
  (net 125 "unconnected-(J601-Pad4)")
  (net 126 "unconnected-(J601-Pad6)")
  (net 127 "unconnected-(J601-Pad7)")
  (net 128 "unconnected-(J601-Pad19)")
  (net 129 "unconnected-(SW101-Pad2)")
  (net 130 "/E-paper display/BUSY")
  (net 131 "/E-paper display/DC")
  (net 132 "Net-(JP301-Pad2)")
  (net 133 "Net-(C509-Pad1)")
  (net 134 "/ESP32-S3-WROOM/GPIO40")
  (net 135 "Net-(J103-Pad2)")
  (net 136 "Net-(J104-Pad8)")
  (net 137 "Net-(J107-Pad1)")
  (net 138 "Fix2")
  (net 139 "Fix1")
  (net 140 "Diss")
  (net 141 "Net-(JP101-Pad2)")
  (net 142 "Net-(JP102-Pad2)")
  (net 143 "Net-(JP103-Pad2)")
  (net 144 "Dis")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.9 78.1 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7224KAHT")
    (property "Radiospares" "788-2997")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C401" (at -7.875 -1 90) (layer "F.SilkS"))
    (fp_text value "220nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C401-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.1 58.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C408" (at -0.05 1.4) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(C408-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.925 63.385 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C411" (at 0.325 -4.615) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C411-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 173.75 65.985 -90)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (property "Mouser" "771-BAT54SW-T/R")
    (property "Radiospares" "380-1216")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "D402" (at 3.465 0.25 180) (layer "F.SilkS"))
    (fp_text value "BAT54SW_SOT323" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(C411-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D402-Pad3)") (pinfunction "K") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" locked (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 164.4 55.9125 -90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "FB402" (at -0.5125 -1.4 90) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0 270) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0 270) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(C408-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.5 78.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0775KL")
    (property "Radiospares" "199-5631")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R401" (at 7.85 0.8 90) (layer "F.SilkS"))
    (fp_text value "75K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(C401-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/SA8x8/In") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.5 78.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-071KL")
    (property "Radiospares" "199-5479")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R402" (at 7.775 1.6 90) (layer "F.SilkS"))
    (fp_text value "1K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C401-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.35 52.85 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100RL")
    (property "Radiospares" "199-5441")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R411" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100R_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(Q403-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SA8x8/SAHL") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.85 64.35 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0717K8L")
    (property "Radiospares" "122-9032")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R415" (at 0.2 3 90) (layer "F.SilkS"))
    (fp_text value "17K8_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C411-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/SA8x8/SAAUDIO_ON") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.5 64.285 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R416" (at 0.215 3.25 90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C411-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(D402-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.05 65.885 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R417" (at -3.315 0.15 90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(D402-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged2Bar12_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 64B54958)
    (at 106.7 67.5 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP601" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Bridged12" (at 0 1.9 90) (layer "F.Fab") hide)
    (fp_text user "3" (at 2.6 0 90) (layer "F.SilkS"))
    (fp_text user "1" (at -2.6 0 90) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 74 "Net-(J601-Pad8)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect locked (at 1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 188.9 107 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (property "Mouser" "771-BC846BW-T/R")
    (property "Radiospares" "436-7931")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q101" (at -1.75 2.6) (layer "F.SilkS"))
    (fp_text value "BC846BW_SOT323" (at -0.05 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 90) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(Q101-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.65 90) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(Q101-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 191.5 106.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100KL")
    (property "Radiospares" "199-5439")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R101" (at 1.1 1.6 90) (layer "F.SilkS"))
    (fp_text value "100K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(Q101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/FORCE_ON") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 183.7 107.7)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100RL")
    (property "Radiospares" "199-5441")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R103" (at -6.5 0.6 180) (layer "F.SilkS"))
    (fp_text value "100R_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(Q102-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(Q101-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.3 102 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R104" (at -1.1 -4.4 -90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/BAT_ADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(Q102-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 183.3 102 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R105" (at -1.2 -4.4 90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/BAT_ADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 181.8 102 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "710-885012206090")
    (property "Radiospares" "839-2969")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C105" (at -1.1 -4.5 90) (layer "F.SilkS"))
    (fp_text value "15nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/BAT_ADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 136.9 103.2 90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Mouser" "241-SS2040FLAUR100A1")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D101" (at 4 0.2 90) (layer "F.SilkS"))
    (fp_text value "SS2040FL_SOD123F" (at 0 2.1 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.4 0 90) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+BATT") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.4 0 90) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/ESP32-S3-WROOM/Boot") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:ESP32-S3-WROOM-1U" (layer "F.Cu")
    (tedit 6496FFE1)
    (at 168.5 97 90)
    (property "Mouser" "356-ESP32S3WM1UN16R2")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "U501" (at 6.85 -10.95 90) (layer "F.SilkS"))
    (fp_text value "ESP32-S3-WROOM-1U" (at 0 12 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.1 -8.05 270) (layer "F.Fab"))
    (pad "" smd roundrect (at -2.9 -2.09 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -2.9 0.71 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.5 0.71 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.1 0.71 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.1 -0.69 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -2.9 -0.69 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.1 -2.09 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.5 -0.69 90) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.5 -2.09 180) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd rect (at -8.75 -8.41 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "2" smd rect (at -8.75 -7.14 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C501-Pad1)") (pinfunction "3v3") (pintype "power_in"))
    (pad "3" smd rect (at -8.75 -5.87 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C503-Pad1)") (pinfunction "En") (pintype "input"))
    (pad "4" smd rect (at -8.75 -4.6 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/ESP32-S3-WROOM/GPIO4") (pinfunction "GPIO4") (pintype "tri_state"))
    (pad "5" smd rect (at -8.75 -3.33 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/ESP32-S3-WROOM/GPIO5") (pinfunction "GPIO5") (pintype "tri_state"))
    (pad "6" smd rect (at -8.75 -2.06 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/ESP32-S3-WROOM/GPIO6") (pinfunction "GPIO6") (pintype "tri_state"))
    (pad "7" smd rect (at -8.75 -0.79 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/ESP32-S3-WROOM/GPIO7") (pinfunction "GPIO7") (pintype "tri_state"))
    (pad "8" smd rect (at -8.75 0.48 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/ESP32-S3-WROOM/GPIO15") (pinfunction "GPIO15") (pintype "tri_state"))
    (pad "9" smd rect (at -8.75 1.75 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/ESP32-S3-WROOM/GPIO16") (pinfunction "GPIO16") (pintype "tri_state"))
    (pad "10" smd rect (at -8.75 3.02 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/ESP32-S3-WROOM/GPIO17") (pinfunction "GPIO17") (pintype "tri_state"))
    (pad "11" smd rect (at -8.75 4.29 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/ESP32-S3-WROOM/GPIO18") (pinfunction "GPIO18") (pintype "tri_state"))
    (pad "12" smd rect (at -8.75 5.56 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/AudioIn") (pinfunction "GPIO8") (pintype "tri_state"))
    (pad "13" smd rect (at -8.75 6.83 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/ESP32-S3-WROOM/D-") (pinfunction "USB_D-") (pintype "tri_state"))
    (pad "14" smd rect (at -8.75 8.1 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/ESP32-S3-WROOM/D+") (pinfunction "USB_D+") (pintype "tri_state"))
    (pad "15" smd rect (at -6.985 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/SQ") (pinfunction "GPIO3") (pintype "tri_state"))
    (pad "16" smd rect (at -5.715 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/FORCE_ON") (pinfunction "GPIO46") (pintype "tri_state"))
    (pad "17" smd rect (at -4.445 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/DC") (pinfunction "GPIO9") (pintype "tri_state"))
    (pad "18" smd rect (at -3.175 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/FSPICS0") (pinfunction "GPIO10") (pintype "tri_state"))
    (pad "19" smd rect (at -1.905 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/BAT_ADC") (pinfunction "GPIO11") (pintype "tri_state"))
    (pad "20" smd rect (at -0.635 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/SW3") (pinfunction "GPIO12") (pintype "tri_state"))
    (pad "21" smd rect (at 0.635 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/SW2") (pinfunction "GPIO13") (pintype "tri_state"))
    (pad "22" smd rect (at 1.905 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "/GPS1PPS") (pinfunction "GPIO14") (pintype "tri_state"))
    (pad "23" smd rect (at 3.175 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/U1RX") (pinfunction "GPIO21") (pintype "tri_state"))
    (pad "24" smd rect (at 4.445 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/U1TX") (pinfunction "GPIO47") (pintype "tri_state"))
    (pad "25" smd rect (at 5.715 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HL") (pinfunction "GPIO48") (pintype "tri_state"))
    (pad "26" smd rect (at 6.985 9.35 90) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/PD") (pinfunction "GPIO45") (pintype "tri_state"))
    (pad "27" smd rect (at 8.75 8.1 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/ESP32-S3-WROOM/GPIO0") (pinfunction "GPIO0") (pintype "tri_state"))
    (pad "28" smd rect (at 8.75 6.83 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/FSPID") (pinfunction "GPIO35") (pintype "tri_state"))
    (pad "29" smd rect (at 8.75 5.56 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/FSSPICLK") (pinfunction "GPIO36") (pintype "tri_state"))
    (pad "30" smd rect (at 8.75 4.29 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Ptt") (pinfunction "GPIO37") (pintype "tri_state"))
    (pad "31" smd rect (at 8.75 3.02 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/BUSY") (pinfunction "GPIO38") (pintype "tri_state"))
    (pad "32" smd rect (at 8.75 1.75 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/GPSRESET") (pinfunction "GPIO39") (pintype "tri_state"))
    (pad "33" smd rect (at 8.75 0.48 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/ESP32-S3-WROOM/GPIO40") (pinfunction "GPIO40") (pintype "tri_state"))
    (pad "34" smd rect (at 8.75 -0.79 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/U2RX") (pinfunction "GPIO41") (pintype "tri_state"))
    (pad "35" smd rect (at 8.75 -2.06 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/U2TX") (pinfunction "GPIO42") (pintype "tri_state"))
    (pad "36" smd rect (at 8.75 -3.33 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Net-(J501-Pad3)") (pinfunction "U0RXD") (pintype "input"))
    (pad "37" smd rect (at 8.75 -4.6 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(J501-Pad2)") (pinfunction "U0TXD") (pintype "output"))
    (pad "38" smd rect (at 8.75 -5.87 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/SW1") (pinfunction "GPIO2") (pintype "input"))
    (pad "39" smd rect (at 8.75 -7.14 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/ESP32-S3-WROOM/GPIO1") (pinfunction "GPIO1") (pintype "input"))
    (pad "40" smd rect (at 8.75 -8.41 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "41" thru_hole circle (at -0.1 0.01 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -1.5 0.01 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole roundrect (at -1.5 -0.7 90) (size 3.7 3.7) (drill 0.25) (layers *.Cu *.Mask) (roundrect_rratio 0.06081081081)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -1.5 -1.39 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -0.8 -2.09 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -0.1 -1.39 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -0.8 0.71 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -0.8 -0.69 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -2.2 -2.09 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -2.2 0.71 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -2.9 0.01 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -2.2 -0.69 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
    (pad "41" thru_hole circle (at -2.9 -1.39 90) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 144 "Dis") (pinfunction "Dis") (pintype "power_in") (zone_connect 2))
  )
  (footprint "_footprint:SA8x8" locked (layer "F.Cu")
    (tedit 64ABFEC4)
    (at 143.2 65)
    (property "G-NiceRF" "SA868")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "U401" (at -0.8 -12.25) (layer "F.SilkS"))
    (fp_text value "SA868" (at -5 -2 -180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at 12.75 0.75) (size 3 2) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 9.25 0.75) (size 3 2) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 9.25 -1.75) (size 3 2) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 12.75 -1.75) (size 3 2) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" np_thru_hole oval locked (at -14 -2.1) (size 2 8) (drill oval 2 8) (layers F&B.Cu *.Mask))
    (pad "1" smd rect locked (at -13.35 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(R414-Pad2)") (pinfunction "Audio_ON") (pintype "output"))
    (pad "2" smd rect locked (at -8.9 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect locked (at -4.45 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D402-Pad3)") (pinfunction "AF_OUT") (pintype "output"))
    (pad "4" smd rect locked (at 0 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect locked (at 4.45 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/SA8x8/SAPTT") (pinfunction "PTT") (pintype "input"))
    (pad "6" smd rect locked (at 8.9 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SA8x8/SAPD") (pinfunction "PD") (pintype "input"))
    (pad "7" smd rect locked (at 13.35 -9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(Q403-Pad3)") (pinfunction "H/L") (pintype "input"))
    (pad "8" smd rect locked (at 17.8 -6.84 90) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "Net-(C408-Pad1)") (pinfunction "VBAT") (pintype "power_in"))
    (pad "9" smd rect locked (at 17.8 -2.24 90) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "10" smd rect locked (at 17.8 2.24 90) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "11" smd rect locked (at 17.8 6.96 90) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "12" smd rect locked (at 13.35 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(J602-Pad1)") (pinfunction "ANT") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 8.9 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "14" smd rect locked (at 4.45 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "15" smd rect locked (at 0 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "16" smd rect locked (at -4.45 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/SA8x8/SARX") (pinfunction "RXD") (pintype "input"))
    (pad "17" smd rect locked (at -8.9 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/SA8x8/SATX") (pinfunction "TXD") (pintype "output"))
    (pad "18" smd rect locked (at -13.35 9.5) (size 1.8 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(C401-Pad1)") (pinfunction "MIC_IN") (pintype "input"))
    (pad "19" smd rect locked (at -17.2 6.4) (size 2.4 9.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Fix2") (pinfunction "Fix2") (pintype "power_in"))
    (pad "20" smd rect locked (at -17.2 -7) (size 2.4 8.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Fix1") (pinfunction "Fix1") (pintype "power_in"))
    (pad "21" thru_hole roundrect locked (at 11 -0.5) (size 8 6) (drill 0.5) (property pad_prop_heatsink) (layers *.Cu *.Mask) (roundrect_rratio 0.08333333333)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (clearance 0.5) (zone_connect 2))
    (pad "21" thru_hole circle locked (at 7.5 -0.5) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 14.5 -0.5) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 11 2) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 14.5 2) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 7.5 2) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 11 -3 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 14.5 -3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
    (pad "21" thru_hole circle locked (at 7.5 -3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 "Diss") (pinfunction "Diss") (pintype "power_in") (zone_connect 2))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 180.42 83.8 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Mouser" " 200-SLW10801GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J103" (at -2.5 2.88 180) (layer "F.SilkS"))
    (fp_text value "SLW-108-01-G-S" (at 0 20.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J103-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/U2TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/U2RX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C110-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/GPSRESET") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/BUSY") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/Ptt") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.7 99.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "C503" (at -0.4 2.8) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C503-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 126.6 88.8 -90)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (property "Mouser" "771-BC846BW-T/R")
    (property "Radiospares" "436-7931")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "Q201" (at -2.3 -3 180) (layer "F.SilkS"))
    (fp_text value "BC846BW_SOT323" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(Q201-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(J204-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:TQFN-10_1.3x1.6mm_P0.4mm" (layer "F.Cu")
    (tedit 64777D0D)
    (at 110.6 93.3)
    (descr "UQFN 10pin, https://www.onsemi.com/pub/Collateral/488AT.PDF")
    (tags "UQFN-10_1.4x1.8mm_P0.4mm")
    (property "Mouser" "729-PI3USB102GZLEX")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "U201" (at -0.6 2 180) (layer "F.SilkS"))
    (fp_text value "PI3USB102G" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.05 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.475 -0.2) (size 0.85 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/USB Charger/USB_P") (pinfunction "Y+") (pintype "input"))
    (pad "2" smd rect locked (at -0.525 0.2) (size 0.75 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/USB Charger/USB_N") (pinfunction "Y-") (pintype "input"))
    (pad "3" smd rect locked (at -0.4 0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "input"))
    (pad "4" smd rect locked (at 0 0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/ESP32-S3-WROOM/D-") (pinfunction "M-") (pintype "input"))
    (pad "5" smd rect locked (at 0.4 0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/ESP32-S3-WROOM/D+") (pinfunction "M+") (pintype "input"))
    (pad "6" smd rect locked (at 0.525 0.2) (size 0.75 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/USB Charger/D-") (pinfunction "D-") (pintype "input"))
    (pad "7" smd rect locked (at 0.525 -0.2) (size 0.75 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/USB Charger/D+") (pinfunction "D+") (pintype "input"))
    (pad "8" smd rect locked (at 0.4 -0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "OE") (pintype "input"))
    (pad "9" smd rect locked (at 0 -0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/USB Charger/Vsys") (pinfunction "Vdd") (pintype "input"))
    (pad "10" smd rect locked (at -0.4 -0.775) (size 0.2 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/USB Charger/INOKB") (pinfunction "Sel") (pintype "input"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-10_1.4x1.8mm_P0.4mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.1 108)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "C501" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SIDELED_APA2107" (layer "F.Cu")
    (tedit 648EA222)
    (at 100.8 102.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Mouser" "604-APA2107LZGCK")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "D203" (at -0.2 2.8 90) (layer "F.SilkS"))
    (fp_text value "APA2107LZGCK" (at 0 1.65 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0.7 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2 0 90) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D203-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.2 0 90) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/USB Charger/Vsys") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.3 101.3 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-072K2L")
    (property "Radiospares" "199-5518")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "R202" (at 0.1 2.5 90) (layer "F.SilkS"))
    (fp_text value "2K2_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/USB Charger/Stat") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 198.2 56.11)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Mouser" "200-HTSW10807GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J108" (at -2.2 11.39 90) (layer "F.SilkS"))
    (fp_text value "HTSW-108-07-G-S" (at 0 20.11) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(J108-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "/L86-M33/GPS1PPS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "/L86-M33/GPSTX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "/L86-M33/GPSRX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/SA8x8/SAHL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/SA8x8/SAPD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "/E-paper display/SDAT") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "/E-paper display/SCLK") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 147.5 103.4 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "FB501" (at -1.3 -1.4) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0 180) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0 180) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.7 101.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "R501" (at 0.5 -3.1) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C503-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1008_2520Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 120.2 88.3)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "81-DFE252012F-1R0MP2")
    (property "Radiospares" "230-7900")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "L201" (at 2.3 -2.3 180) (layer "F.SilkS"))
    (fp_text value "DFE252012F-1R0M" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.075 0) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 6 "Net-(C204-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.075 0) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 88 "/USB Charger/Vsys") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.5 96.85 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C201" (at -8.45 0.3 90) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.2 96.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "R205" (at 3.55 -0.2 90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(J204-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C203-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.8 91.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C206" (at -8.9 0.7 90) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/USB Charger/Vsys") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.3 85.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C204" (at -1.3 1.1) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C204-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.9 83.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C209" (at -3.3 -0.1) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C207-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.9 85.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C207" (at -3.2 0) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C207-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.4 87.925 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BBJ225KA-T")
    (property "Radiospares" "103-4115")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C202" (at 0.425 -3 90) (layer "F.SilkS"))
    (fp_text value "2.2µF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.3 90.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BBJ225KA-T")
    (property "Radiospares" "103-4115")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C205" (at 1 1.2) (layer "F.SilkS"))
    (fp_text value "2.2µF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C205-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.9 87.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C210" (at -3.2 -1) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C207-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.7 96.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "R203" (at 3.45 0 90) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:FC2QFN-24_3x3_Pitch0.4mm" (layer "F.Cu")
    (tedit 648739E3)
    (at 115.3 92.1)
    (descr "Maxim F243A3F ")
    (tags "FC2QFN F243A3F MAX77751 MAX77757")
    (property "Mouser" "700-MAX77757JEFG420")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "U202" (at -3 0.7 90) (layer "F.SilkS"))
    (fp_text value "MAX77757CEFG+" (at 0 3.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd custom locked (at -1.8 -1) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C204-Pad1)") (pinfunction "BST") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.513 -0.1)
            (xy 0.625 -0.012)
            (xy 0.625 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom locked (at -1.8 -0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/USB Charger/INOKB") (pinfunction "INOKB") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "3" smd custom locked (at -1.8 -0.2) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/USB Charger/Stat") (pinfunction "STAT") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "4" smd custom locked (at -1.8 0.2) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J202-PadB5)") (pinfunction "CC2") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "5" smd custom locked (at -1.8 0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J202-PadA5)") (pinfunction "CC1") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "6" smd custom locked (at -1.8 1 180) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/USB Charger/D+") (pinfunction "DP") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy -0.513 -0.1)
            (xy -0.625 -0.012)
            (xy -0.625 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
      ))
    (pad "7" smd custom locked (at -1 1.8 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/USB Charger/D-") (pinfunction "DN") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.513 -0.1)
            (xy 0.625 -0.012)
            (xy 0.625 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
      ))
    (pad "8" smd custom locked (at -0.6 1.8 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/USB Charger/ENBST") (pinfunction "ENBST") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "9" smd custom locked (at -0.2 1.8 180) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Gnd") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.1 0)
            (xy -0.1 1.225)
            (xy 0.1 1.225)
            (xy 0.1 0)
          ) (width 0) (fill yes))
            (gr_circle (center 0 1.225) (end 0.1 1.225) (width 0) (fill yes))
      ))
    (pad "10" smd custom locked (at 0.2 1.8 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C203-Pad1)") (pinfunction "Vdd") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "11" smd custom locked (at 0.6 1.8 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(J204-Pad1)") (pinfunction "THM") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "12" smd custom locked (at 1 1.8 270) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(R203-Pad1)") (pinfunction "IFAST") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy -0.513 -0.1)
            (xy -0.625 -0.012)
            (xy -0.625 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
      ))
    (pad "13" smd custom locked (at 1.8 1) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(C201-Pad1)") (pinfunction "BAT") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 0.1)
            (xy -0.488 0.1)
            (xy -0.65 -0.062)
            (xy -0.65 -0.25)
            (xy -1.475 -0.25)
            (xy -1.475 -0.5)
            (xy 0 -0.5)
          ) (width 0) (fill yes))
            (gr_circle (center -1.475 -0.4) (end -1.375 -0.4) (width 0) (fill yes))
            (gr_circle (center -1.475 -0.35) (end -1.375 -0.35) (width 0) (fill yes))
            (gr_poly (pts
            (xy -1.575 -0.4)
            (xy -1.575 -0.35)
            (xy -1.475 -0.35)
            (xy -1.475 -0.4)
          ) (width 0) (fill yes))
      ))
    (pad "14" smd circle locked (at 1.8 0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(C201-Pad1)") (pinfunction "BAT") (pintype "input") (zone_connect 2))
    (pad "15" smd custom locked (at 1.8 0.2) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/USB Charger/Vsys") (pinfunction "SYS") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.5)
            (xy -0.55 -0.5)
            (xy -0.65 -0.4)
            (xy -0.65 -0.15)
            (xy -1.475 -0.15)
            (xy -1.575 -0.05)
            (xy -1.575 0)
            (xy -1.475 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center -1.475 0) (end -1.375 0) (width 0) (fill yes))
            (gr_circle (center -1.475 -0.05) (end -1.375 -0.05) (width 0) (fill yes))
            (gr_circle (center -0.55 -0.4) (end -0.45 -0.4) (width 0) (fill yes))
      ))
    (pad "16" smd circle locked (at 1.8 -0.2) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/USB Charger/Vsys") (pinfunction "SYS") (pintype "input") (zone_connect 2))
    (pad "17" smd custom locked (at 1.8 -0.6 180) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C205-Pad1)") (pinfunction "PVL") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.1)
            (xy 0.575 -0.1)
            (xy 0.675 0)
            (xy 0.575 0.1)
            (xy 0 0.1)
          ) (width 0) (fill yes))
            (gr_circle (center 0.575 0) (end 0.675 0) (width 0) (fill yes))
      ))
    (pad "18" smd custom locked (at 1.8 -1) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PGND") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 0.1)
            (xy -0.8 0.1)
            (xy -0.9 0)
            (xy -0.9 -0.8)
            (xy -0.7 -0.8)
            (xy -0.7 -0.35)
            (xy -0.45 -0.1)
            (xy 0 -0.1)
          ) (width 0) (fill yes))
            (gr_circle (center -0.8 0) (end -0.7 0) (width 0) (fill yes))
      ))
    (pad "19" smd circle locked (at 1 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PGND") (pintype "input") (zone_connect 2))
    (pad "20" smd custom locked (at 0.6 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C204-Pad2)") (pinfunction "LX") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.5 0)
            (xy -0.5 0.975)
            (xy -0.4 1.075)
            (xy 0 1.075)
            (xy 0.1 0.975)
            (xy 0.1 0)
          ) (width 0) (fill yes))
            (gr_circle (center -0.4 0.975) (end -0.3 0.975) (width 0) (fill yes))
            (gr_circle (center 0 0.975) (end 0.1 0.975) (width 0) (fill yes))
      ))
    (pad "21" smd circle locked (at 0.2 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C204-Pad2)") (pinfunction "LX") (pintype "input") (zone_connect 2))
    (pad "22" smd custom locked (at -0.2 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C207-Pad1)") (pinfunction "BYP") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.1 0)
            (xy -0.1 0.975)
            (xy 0.1 0.975)
            (xy 0.1 0)
          ) (width 0) (fill yes))
            (gr_circle (center 0 0.975) (end 0.1 0.975) (width 0) (fill yes))
      ))
    (pad "23" smd custom locked (at -0.6 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "CHGIN") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -0.5 0)
            (xy -0.5 0.488)
            (xy -0.388 0.6)
            (xy -0.15 0.6)
            (xy -0.15 0.975)
            (xy -0.05 1.075)
            (xy 0 1.075)
            (xy 0.1 0.975)
            (xy 0.1 0)
          ) (width 0) (fill yes))
            (gr_circle (center 0 0.975) (end 0.1 0.975) (width 0) (fill yes))
            (gr_circle (center -0.05 0.975) (end 0.05 0.975) (width 0) (fill yes))
      ))
    (pad "24" smd circle locked (at -1 -1.8) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "CHGIN") (pintype "input") (zone_connect 2))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.8 91.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C208" (at -8.8 0.05 90) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/USB Charger/Vsys") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 180.4 51.8 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Mouser" "200-HTSW10807GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J106" (at -2.3 4.7) (layer "F.SilkS"))
    (fp_text value "HTSW-108-07-G-S" (at 0 20.11 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/SA8x8/Out") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/SA8x8/SAAUDIO_ON") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "/E-paper display/PON") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "/E-paper display/CS") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "/E-paper display/DC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(J106-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 189.9 56.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "C304" (at 0 2.4 270) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C303-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SKTDLDE010" (layer "F.Cu")
    (tedit 0)
    (at 120.1 80)
    (property "Mouser" "688-SKTDLDE010")
    (property "Radiospares" "917-3839")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at -4.1 -0.7 unlocked) (layer "F.SilkS"))
    (fp_text value "SKTDLDE010" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(J106-Pad8)") (pinfunction "B") (pintype "passive"))
    (pad "S" thru_hole custom (at -1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask "F.Paste") (remove_unused_layers) (keep_end_layers)
      (net 143 "Net-(JP103-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy -0.25 -0.2)
            (xy -0.25 0.75)
            (xy 0.5 0.75)
            (xy 0.5 0.4)
            (xy 0.2 0.4)
            (xy 0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
    (pad "S" thru_hole custom (at 1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask)
      (net 143 "Net-(JP103-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy 0.25 -0.2)
            (xy 0.25 0.75)
            (xy -0.5 0.75)
            (xy -0.5 0.4)
            (xy -0.2 0.4)
            (xy -0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
    (pad "S" smd roundrect (at 0 -2.45) (size 1.4 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(JP103-Pad2)") (pinfunction "MP") (pintype "free"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.64 56.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C607" (at 3.35 0 270) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(C607-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.34 61.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C602" (at -4.06 -1.7) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SKTDLDE010" (layer "F.Cu")
    (tedit 0)
    (at 136.25 80)
    (property "Mouser" "688-SKTDLDE010")
    (property "Radiospares" "917-3839")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at -3.25 -1.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "SKTDLDE010" (at 0 0.95 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(J108-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "S" smd roundrect (at 0 -2.45) (size 1.4 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(JP102-Pad2)") (pinfunction "MP") (pintype "free"))
    (pad "S" thru_hole custom (at 1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask)
      (net 142 "Net-(JP102-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy 0.25 -0.2)
            (xy 0.25 0.75)
            (xy -0.5 0.75)
            (xy -0.5 0.4)
            (xy -0.2 0.4)
            (xy -0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
    (pad "S" thru_hole custom (at -1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask "F.Paste") (remove_unused_layers) (keep_end_layers)
      (net 142 "Net-(JP102-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy -0.25 -0.2)
            (xy -0.25 0.75)
            (xy 0.5 0.75)
            (xy 0.5 0.4)
            (xy 0.2 0.4)
            (xy 0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109.64 73.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C604" (at 3.3 -0.1 180) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(C506-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 112.84 56.325 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C610" (at 3.625 -0.04 270) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(C610-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 111.19 76.3 -90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Mouser" "241-SS2040FLAUR100A1")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "D605" (at -0.2 5.65 90) (layer "F.SilkS"))
    (fp_text value "SS2040FL_SOD123F" (at 0 2.1 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.05 5.4 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(C611-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 187.25 56.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "C303" (at 3.25 0.05 180) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C303-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 184.45 61.7 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "FB301" (at 3.75 -0.1) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0 180) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0 180) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.34 63.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C603" (at 3.96 1.3) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SKTDLDE010" (layer "F.Cu")
    (tedit 0)
    (at 152.4 80)
    (property "Mouser" "688-SKTDLDE010")
    (property "Radiospares" "917-3839")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 3.6 -1.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "SKTDLDE010" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(J105-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 -2.3) (size 0.7 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "B") (pintype "passive"))
    (pad "S" thru_hole custom (at 1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask)
      (net 141 "Net-(JP101-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy 0.25 -0.2)
            (xy 0.25 0.75)
            (xy -0.5 0.75)
            (xy -0.5 0.4)
            (xy -0.2 0.4)
            (xy -0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
    (pad "S" thru_hole custom (at -1.85 -0.95) (size 0.9 0.9) (drill 0.55) (layers *.Cu *.Mask "F.Paste") (remove_unused_layers) (keep_end_layers)
      (net 141 "Net-(JP101-Pad2)") (pinfunction "MP") (pintype "free")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0 -0.2)
            (xy -0.25 -0.2)
            (xy -0.25 0.75)
            (xy 0.5 0.75)
            (xy 0.5 0.4)
            (xy 0.2 0.4)
            (xy 0.2 0)
            (xy 0 0)
          ) (width 0.4) (fill yes))
      ))
    (pad "S" smd roundrect (at 0 -2.45) (size 1.4 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(JP101-Pad2)") (pinfunction "MP") (pintype "free"))
  )
  (footprint "_footprint:JST_S2B-ZR-SM4A-TF_1x02-1MP_P1.50mm_Horizontal" (layer "F.Cu")
    (tedit 5C2814BC)
    (at 191.9 62.175)
    (descr "JST ZE series connector, SM02B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
    (tags "connector JST ZE horizontal")
    (property "Farnell" "1830920")
    (property "Mouser" "306-S2BZRSM4ATFLFSN")
    (property "Radiospares" "762-0875")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "J302" (at -0.4 4.925) (layer "F.SilkS"))
    (fp_text value "S2B-ZR-SM4A-TF" (at 0 6.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.75 -2.575) (size 0.7 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.75 -2.575) (size 0.7 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C303-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.7 1.125) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388890909)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.7 1.125) (size 1.1 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388890909)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_ZE_SM02B-ZESS-TB_1x02-1MP_P1.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.24 56.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C608" (at 3.4 -0.05 270) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(C608-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SOT-323T_SC-113A" (layer "F.Cu")
    (tedit 648484CB)
    (at 116.14 72.85 -90)
    (descr "SOT-323, SC-70, TUMT3")
    (tags "SOT-323 SC-70")
    (property "Mouser" "755-RTF025N03TL")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "Q603" (at 0.15 -1.76 -90) (layer "F.SilkS"))
    (fp_text value "RTF025N03TL" (at -0.05 2.05 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.85 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(J601-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -0.85 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(J601-Pad3)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 0.85 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(C611-Pad1)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 108.79 76.3 -90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Mouser" "241-SS2040FLAUR100A1")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "D604" (at -0.2 4.65 -90) (layer "F.SilkS"))
    (fp_text value "SS2040FL_SOD123F" (at 0 2.1 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.05 4.2 -90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "Net-(C506-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(C611-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:Hirose_FH34-24SRJ-0.5SH_1x24-1MP_P0.50mm_Horizontal" locked (layer "F.Cu")
    (tedit 64B29E86)
    (at 111.14 65.2 -90)
    (descr "Hirose FH12, FFC/FPC connector, FH12-24S-0.5SH, 24 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Mouser" "798-FH34SRJ24S05SH99")
    (property "Radiospares" "136-2403")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "J601" (at -5.6 3.55) (layer "F.SilkS"))
    (fp_text value "FH34SRJ-24S-05SH" (at 0 5.6 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.1 0.1 90) (layer "F.Fab"))
    (pad "" smd rect locked (at 1.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -2.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 5.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 5.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 2.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 3.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -5.75 -1.85 270) (size 0.3 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 4.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 3.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -1.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -3.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -5.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -4.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 4.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -1.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -4.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 2.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -2.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at 1.75 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "" smd rect locked (at -3.25 -1.85 270) (size 0.25 0.65) (layers "F.Paste"))
    (pad "1" smd rect locked (at 5.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "unconnected-(J601-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" smd rect locked (at 5.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(J601-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at 4.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(J601-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at 4.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "unconnected-(J601-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" smd rect locked (at 3.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(C606-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at 3.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "unconnected-(J601-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" smd rect locked (at 2.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "unconnected-(J601-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" smd rect locked (at 2.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(J601-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 1.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/E-paper display/BUSY") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 1.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(C601-Pad1)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 0.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/E-paper display/DC") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 0.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "/E-paper display/CS") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at -0.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "/E-paper display/SCLK") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at -0.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "/E-paper display/SDAT") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at -1.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at -1.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at -2.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at -2.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(C607-Pad1)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at -3.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "unconnected-(J601-Pad19)") (pinfunction "Pin_19") (pintype "passive+no_connect"))
    (pad "20" smd rect locked (at -3.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(C608-Pad1)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at -4.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "Net-(C506-Pad2)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at -4.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(C609-Pad1)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at -5.25 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "Net-(C507-Pad2)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at -5.75 -1.85 270) (size 0.3 0.8) (drill (offset 0 0.075)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(C610-Pad1)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "MP" smd rect locked (at 6.75 0.725 270) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd rect locked (at -6.75 0.725 270) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-24S-0.5SH_1x24-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical" (layer "F.Cu")
    (tedit 5A1DBFC3)
    (at 181.7 73.9 -90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (property "Mouser" "798-U.FL-R-SMT-110")
    (property "Radiospares" "557-981")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "J301" (at -2.8 0.1) (layer "F.SilkS"))
    (fp_text value "U.FL-R-SMT-1" (at 0.475 3.2 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.475 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.05 0 270) (size 1.05 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J301-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 1.475 270) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 -1.475 270) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl"
      (offset (xyz 0.4749999928 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109.44 56.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C609" (at 3.3 0.06 270) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(C609-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:Inductor_Pulse_PA4322.xxxNLT_5.1x5.1" locked (layer "F.Cu")
    (tedit 648452B1)
    (at 121.35 72.2 180)
    (property "Mouser" "673-PA4322.103NLT")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr through_hole)
    (fp_text reference "L601" (at 0.1 0.05 180) (layer "F.SilkS"))
    (fp_text value "PA4322.103NLT" (at 0 -0.5 180) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 -2.55 180) (size 5.08 2.54) (drill (offset 0 0.4)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(C611-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 0 2.55) (size 5.08 2.54) (drill (offset 0 0.4)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.04 70)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "71-RCWE0805R470FKEA")
    (property "Radiospares" "199-6016")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "R606" (at 0.16 -3.1) (layer "F.SilkS"))
    (fp_text value "0R47_0805" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439004878)
      (net 75 "Net-(J601-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439004878)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.84 68.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C606" (at 0.36 -2.5 -180) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 -180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(C606-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 184.2 57.95 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "C301" (at 3.1 -0.1 180) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.24 73.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C605" (at 5.55 1.25 180) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(C507-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 113.59 76.3 90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Mouser" "241-SS2040FLAUR100A1")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "D606" (at 0.2 -6.65 90) (layer "F.SilkS"))
    (fp_text value "SS2040FL_SOD123F" (at 0 2.1 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.05 -6.7 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.4 0 90) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(C611-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.4 0 90) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "Net-(C507-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.79 76.45 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "81-GRM21BR61H475KE1L")
    (property "Radiospares" "113-8707")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C611" (at 0.35 -1.61 -90) (layer "F.SilkS"))
    (fp_text value "4.7µF_0805" (at 0 1.68 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(C611-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(C611-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.6 61.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C601" (at -0.1 9.1 270) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C601-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 126.4 52.3)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "FB601" (at 0.1 -1.5) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(C504-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+BATT") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.075 63.385)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "710-885012206094")
    (property "Radiospares" "839-2978")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C405" (at 3.575 0.115) (layer "F.SilkS"))
    (fp_text value "68nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SA8x8/Out") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SOT-323T_SC-113A" (layer "F.Cu")
    (tedit 648484CB)
    (at 159.15 52.95 -90)
    (descr "SOT-323, SC-70, TUMT3")
    (tags "SOT-323 SC-70")
    (property "Mouser" "755-RTF025N03TL")
    (property "Radiospares" "")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "Q403" (at -1.9 0.1 180) (layer "F.SilkS"))
    (fp_text value "RTF025N03TL" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.85 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(Q403-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -0.85 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 0.85 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(Q403-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.85 65.81 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0722RL")
    (property "Radiospares" "199-5504")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R404" (at 3.54 0.05 90) (layer "F.SilkS"))
    (fp_text value "22R_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SA8x8/Out") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(D402-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.5 86.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100KL")
    (property "Radiospares" "199-5439")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "R204" (at -1.1 1.4) (layer "F.SilkS"))
    (fp_text value "100K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(Q201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/USB Charger/CHGOFF") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:USB_C_Receptacle_GCT_4105" (layer "F.Cu")
    (tedit 64AD0F2D)
    (at 103.74 90.9 -90)
    (descr "http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf")
    (tags "USB C Type-C Receptacle USB2.0")
    (property "Mouser" "640-USB4105-GF-A-120")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "J202" (at 6 0.24 180) (layer "F.SilkS"))
    (fp_text value "USB4105-GF-A-120" (at 0 6.24 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.18 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 90) (size 0.6 0.6) (drill 0.6) (layers "Dwgs.User")
      (clearance 0.01))
    (pad "" np_thru_hole circle (at -2.89 -1.45 90) (size 0.6 0.6) (drill 0.6) (layers F&B.Cu *.Mask)
      (zone_connect 0))
    (pad "A1" smd rect (at -3.2 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.4 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J202-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/USB Charger/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/USB Charger/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "unconnected-(J202-PadA8)") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 2.4 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.2 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.2 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.4 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J202-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/USB Charger/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/USB Charger/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -2.51 90) (size 0.3 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "unconnected-(J202-PadB8)") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" smd rect (at -2.4 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.2 -2.51 270) (size 0.6 1.16) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 2.24) (size 1.7 0.95) (drill oval 1.4 0.6) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 2.24) (size 1.7 0.95) (drill oval 1.4 0.6) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 -1.93) (size 2 0.95) (drill oval 1.7 0.6) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 -1.93) (size 2 0.95) (drill oval 1.7 0.6) (layers *.Cu *.Mask "F.Paste")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Palconn_UTC16-G.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.95 104.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C101" (at -0.25 -15.6) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.7 102.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C102" (at -0.1 -15.3) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C101-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.9 102.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C103" (at 0.4 15.2) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.5 104.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C104" (at 0 15.6) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 141.8 97 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Mouser" "621-AP7361C-33E-13")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U101" (at 11.4 0 180) (layer "F.SilkS"))
    (fp_text value "AP7361C-33E_SOT223" (at 0 4.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C101-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at 3.15 0 90) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -3.15 2.3 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.1 83.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100KL")
    (property "Radiospares" "199-5439")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "R201" (at 3.3 0.2) (layer "F.SilkS"))
    (fp_text value "100K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/USB Charger/Vsys") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/USB Charger/INOKB") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.6 96.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BBJ225KA-T")
    (property "Radiospares" "103-4115")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C203" (at 0.1 1.3 90) (layer "F.SilkS"))
    (fp_text value "2.2µF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.6 107.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R102" (at 7.5 -0.5 180) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(Q102-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 180.42 78.2 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Mouser" "200-HTSW10807GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J105" (at 2.25 8.68 180) (layer "F.SilkS"))
    (fp_text value "HTSW-108-07-G-S" (at 0 20.11 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(J105-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/SA8x8/SARX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/SA8x8/SATX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/SA8x8/In") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "/L86-M33/GPSRESET") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "/E-paper display/BUSY") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/SA8x8/SAPTT") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.9 56.15)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C106" (at 0.3 1.65) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(C106-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.85 53.575 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C107" (at 2.675 -0.95 180) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(C106-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 168.425 52.15 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C108" (at -0.175 1.3) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 168.85 54.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C109" (at -0.05 -1.5 90) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (tedit 5C33D6E8)
    (at 172.5 54.5125 -90)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Mouser" "865-XC6206P332PR-G")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U102" (at 3.1375 -0.7 180) (layer "F.SilkS"))
    (fp_text value "XC6206P332PR_SOT89" (at 0.3 3.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.5 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.65 -1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd custom locked (at -1.5625 0 270) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(C106-Pad1)") (pinfunction "VI") (pintype "power_in") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
          ) (width 0) (fill yes))
      ))
    (pad "3" smd rect locked (at -1.65 1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 198.2 105.89 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Mouser" " 200-SLW10801GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J107" (at 3.5 2.59 270) (layer "F.SilkS"))
    (fp_text value "SLW-108-01-G-S" (at 0 20.55 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89 270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J107-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "/GPS1PPS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "/U1RX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/U1TX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/HL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/PD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/FSPID") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/FSSPICLK") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323F" (layer "F.Cu")
    (tedit 590A48EB)
    (at 150.4 102.4 90)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags "SOD-323F")
    (property "Mouser" "771-BAT54J115")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "D501" (at 0 1.8 90) (layer "F.SilkS"))
    (fp_text value "BAT54J_SOD323F" (at 0.1 1.9 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.1 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 0 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C501-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.1 0 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C503-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 180.42 110.2 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Mouser" " 200-SLW10801GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J104" (at 2 13.48 180) (layer "F.SilkS"))
    (fp_text value "SLW-108-01-G-S" (at 0 20.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/AudioIn") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/SQ") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "/FORCE_ON") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "/FSPICS0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "/DC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(J104-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.7 108 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "C502" (at -3.4 -0.25) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0.125 1.3) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SOT-323T_SC-113A" (layer "F.Cu")
    (tedit 648484CB)
    (at 180.8 105.2 90)
    (descr "SOT-323, SC-70, TUMT3")
    (tags "SOT-323 SC-70")
    (property "Mouser" "755-RZF020P01TL")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q102" (at -0.1 1.9 270) (layer "F.SilkS"))
    (fp_text value "RZF020P01TL" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.85 -0.65) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(Q102-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -0.85 0.65) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+BATT") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 0.85 0) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(Q102-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 177.6 52.95 -90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB102" (at -0.65 -1.3 90) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0 270) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0 270) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(C106-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.2 78.1 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "80-C0603C472K5R")
    (property "Radiospares" "264-4589")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C402" (at -7.9 -1.3 90) (layer "F.SilkS"))
    (fp_text value "4.7nF_50V_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323F" (layer "F.Cu")
    (tedit 590A48EB)
    (at 187.3 62 -90)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags "SOD-323F")
    (property "Mouser" "771-BAT54J115")
    (property "Radiospares" "")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "D301" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "BAT54J_SOD323F" (at 0.1 1.9 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.8 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(D301-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C301-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.9 60.585 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "C404" (at 1.215 2.5 180) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C404-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.2 52.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100RL")
    (property "Radiospares" "199-5441")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "R414" (at -0.5 1.55) (layer "F.SilkS"))
    (fp_text value "100R_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q406-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(R414-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.3 60.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "")
    (property "Radiospares" "")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "R607" (at 0.15 1.45 90) (layer "F.SilkS"))
    (fp_text value "R_DNP_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C404-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q406-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 187.1 58.825 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-071KL")
    (property "Radiospares" "199-5479")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "R301" (at 0.325 1.2 90) (layer "F.SilkS"))
    (fp_text value "1K_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(D301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C303-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.575 52.5625)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C504" (at -0.375 -1.6625) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(C504-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 121.6 57.7 -90)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (property "Mouser" "771-BAT54SW-T/R")
    (property "Radiospares" "380-1216")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "D601" (at 2.5 -9.7 90) (layer "F.SilkS"))
    (fp_text value "BAT54SW_SOT323" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(C601-Pad1)") (pinfunction "K") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.2 60.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0710KL")
    (property "Radiospares" "199-5443")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "R604" (at -0.2 1.5) (layer "F.SilkS"))
    (fp_text value "10K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(C601-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.8 67.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C505" (at -0.5 -1.7) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.84 56.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C506" (at -3.3 -0.06 90) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(C506-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.14 56.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C507" (at -3.2 -0.06 90) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(C507-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 170.25 58.85 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "FB401" (at 0 -1.55 90) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0 90) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C404-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0 90) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SOT-323T_SC-113A" (layer "F.Cu")
    (tedit 648484CB)
    (at 174.1 60.785 -90)
    (descr "SOT-323, SC-70, TUMT3")
    (tags "SOT-323 SC-70")
    (property "Mouser" "755-RZF020P01TL")
    (property "Radiospares" "")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "Q406" (at -1.835 -0.25 180) (layer "F.SilkS"))
    (fp_text value "RZF020P01TL" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.85 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(Q406-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -0.85 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C404-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 0.85 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/SA8x8/SAAUDIO_ON") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 184.4 59.75 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-TMK212BBJ106MG-T")
    (property "Radiospares" "184-3756")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "C302" (at 3.4 -0.15 180) (layer "F.SilkS"))
    (fp_text value "10µF_0805" (at 0 1.68 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C301-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:SW_PCM13SMTR _SP3T" (layer "F.Cu")
    (tedit 64860296)
    (at 141 110.5)
    (descr "Switch SMD SP3T")
    (property "Mouser" "611-PCM13SMTR ")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW101" (at 0 0.5) (layer "F.SilkS"))
    (fp_text value "PCM13SMTR" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 3 0) (size 1 1) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3 0) (size 1 1) (drill 0.95) (layers *.Cu *.Mask))
    (pad "1" smd rect (at -3 -1.75) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/ESP32-S3-WROOM/Boot") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -1.5 -1.75) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "unconnected-(SW101-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.5 -1.75) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/USB Charger/Vsys") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 3 -1.75) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+BATT") (pinfunction "4") (pintype "passive"))
    (pad "MP" smd rect (at 5 -0.965) (size 0.7 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MP") (pintype "input"))
    (pad "MP" smd rect (at 5 0.965) (size 0.7 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MP") (pintype "input"))
    (pad "MP" smd rect (at -5 0.965) (size 0.7 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MP") (pintype "input"))
    (pad "MP" smd rect (at -5 -0.965) (size 0.7 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "MP") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.9 106.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-07100KL")
    (property "Radiospares" "199-5439")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "R504" (at -0.6 16.2) (layer "F.SilkS"))
    (fp_text value "100K_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(Q501-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/ESP32-S3-WROOM/Boot") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical" (layer "F.Cu")
    (tedit 5A1DBFC3)
    (at 165.3 75.95)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (property "Mouser" "798-U.FL-R-SMT-110")
    (property "Radiospares" "557-981")
    (property "Sheetfile" "SA8x8.kicad_sch")
    (property "Sheetname" "SA8x8")
    (attr smd)
    (fp_text reference "J602" (at 3.6 0.05 90) (layer "F.SilkS"))
    (fp_text value "U.FL-R-SMT-1" (at 0.475 3.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.475 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.05 0) (size 1.05 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(J602-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 -1.475) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 1.475) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl"
      (offset (xyz 0.4749999928 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 114.1 51.6)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "REF1" (at 0.8 1.3) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle locked (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 191 94)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "REF2" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle locked (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 102.7 106.5)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "REF3" (at 2.5 0.2 180) (layer "F.SilkS"))
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Diode_SMD:D_SOD-323F" (layer "F.Cu")
    (tedit 590A48EB)
    (at 141.7 106.2)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags "SOD-323F")
    (property "Mouser" "771-BAT54J115")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D102" (at -0.2 -16.3) (layer "F.SilkS"))
    (fp_text value "BAT54J_SOD323F" (at 0.1 1.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.2 1.6) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 0) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C101-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.1 0) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323F" (layer "F.Cu")
    (tedit 590A48EB)
    (at 179.75 55.35 -90)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags "SOD-323F")
    (property "Mouser" "771-BAT54J115")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D103" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "BAT54J_SOD323F" (at 0.05 1.95 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(C106-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 128.65 96.5)
    (descr "JST PH series connector, S3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Mouser" "306-S3BPHSM4TBLFSN")
    (property "Radiospares" "688-1357")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "J204" (at 4.45 -4.3) (layer "F.SilkS"))
    (fp_text value "S3B-PH-SM4-TB" (at 0 5.8 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(J204-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C201-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 2 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "MP" smd roundrect (at -4.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at 4.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 137.9 106.4)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Mouser" "710-742792031")
    (property "Radiospares" "669-4092")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB101" (at -0.7 -16.1) (layer "F.SilkS"))
    (fp_text value "WE-CBF_742792031" (at 0 1.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C101-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 147.9 106.9 -90)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (property "Mouser" "771-BC846BW-T/R")
    (property "Radiospares" "436-7931")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr smd)
    (fp_text reference "Q501" (at 0.7 -3.4) (layer "F.SilkS"))
    (fp_text value "BC846BW_SOT323" (at -0.05 2.05 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(Q501-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.45 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/ESP32-S3-WROOM/GPIO0") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434)
    (at 101.8 51.8 90)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Mouser" " 200-SLW10101GS")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J111" (at -2.2 0.3 180) (layer "F.SilkS"))
    (fp_text value "SLW-101-01-G-S" (at 0 2.77 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.6 106.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0747KL")
    (property "Radiospares" "199-5581")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R106" (at 3.5 0.1) (layer "F.SilkS"))
    (fp_text value "47K_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/ESP32-S3-WROOM/Boot") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163.4 86.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R108" (at 3.1 0.1) (layer "F.SilkS"))
    (fp_text value "470R_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "/SW1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(J103-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.7 97.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R110" (at 3.5 0) (layer "F.SilkS"))
    (fp_text value "470R_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/SW3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(J104-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 101.8 83.8)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Mouser" "200-HTSW10107GS")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J110" (at 2.2 0.8 90) (layer "F.SilkS"))
    (fp_text value "HTSW-101-07-G-S" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A434)
    (at 101.8 78.2 180)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Mouser" " 200-SLW10101GS")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J112" (at -2.9 -0.6) (layer "F.SilkS"))
    (fp_text value "SLW-101-01-G-S" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.5 56 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C509" (at 0 -1.3 90) (layer "F.SilkS"))
    (fp_text value "10nF_50V_0603" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C509-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 118.1 55.5 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "U502" (at -3 2.6 -90) (layer "F.SilkS"))
    (fp_text value "LP2985-3.3" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(C504-Pad2)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/E-paper display/PON") (pinfunction "ON/~{OFF}") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C509-Pad1)") (pinfunction "BP") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.6 78.3 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JP102" (at -0.7 -1.5 -90) (layer "F.SilkS"))
    (fp_text value "DNP 0603" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(J108-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(JP102-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.4 58.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107BJ105KA-T")
    (property "Radiospares" "103-4112")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C510" (at -0.7 1.5) (layer "F.SilkS"))
    (fp_text value "1µF_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(C505-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 195.1 73.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-0747KL")
    (property "Radiospares" "199-5581")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R111" (at 4.5 -0.3 90) (layer "F.SilkS"))
    (fp_text value "47K_0603" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/E-paper display/PON") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.9 86.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "603-RC0603FR-071KL")
    (property "Radiospares" "199-5479")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R107" (at 3.5 -1.6) (layer "F.SilkS"))
    (fp_text value "1K_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "/ESP32-S3-WROOM/GPIO40") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C110-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.9 84.7 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "80-C0603C472K5R")
    (property "Radiospares" "264-4589")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C110" (at -3.5 -1.5) (layer "F.SilkS"))
    (fp_text value "4.7nF_50V_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C110-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.8 87.925 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C214" (at 0.325 -2.7 90) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.425 94.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C211" (at 0.575 8.7) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5B391E66)
    (at 192.9 71.1 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP301" (at -0.2 2.1 -90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 -90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 100 "/E-paper display/PON") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 132 "Net-(JP301-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.4 54 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "81-GRM21BR61H475KE1L")
    (property "Radiospares" "113-8707")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "C508" (at 1.6 -9.4 90) (layer "F.SilkS"))
    (fp_text value "4.7µF_0805" (at -6.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(C504-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.7 96.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R109" (at 3.6 0.1) (layer "F.SilkS"))
    (fp_text value "470R_0603" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/SW2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(J107-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 101.8 110.2 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Mouser" "200-HTSW10107GS")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J109" (at 0 2 180) (layer "F.SilkS"))
    (fp_text value "HTSW-101-07-G-S" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323F" (layer "F.Cu")
    (tedit 590A48EB)
    (at 121.2 54.2 -90)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags "SOD-323F")
    (property "Mouser" "771-BAT54J115")
    (property "Radiospares" "")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr smd)
    (fp_text reference "D502" (at 1.3 -10.2 90) (layer "F.SilkS"))
    (fp_text value "BAT54J_SOD323F" (at 0.1 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "Net-(C504-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0 270) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(C505-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.6 88.675 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C213" (at 0 -1.2 90) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/USB Charger/Vsys") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.8 88.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Mouser" "963-UMK107B7104KAHT")
    (property "Radiospares" "184-3685")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "C212" (at -4.9 1.3) (layer "F.SilkS"))
    (fp_text value "100nF_0603" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C207-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.5 78.3 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JP103" (at 0.4 -1.5 -90) (layer "F.SilkS"))
    (fp_text value "DNP 0603" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(J106-Pad8)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(JP103-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149 78.4 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JP101" (at -0.9 3 -90) (layer "F.SilkS"))
    (fp_text value "DNP 0603" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(J105-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(JP101-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A41D)
    (at 148.67 110.2 -90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (property "Mouser" "200-SSQ11201GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at -1.9 1.17) (layer "B.SilkS"))
    (fp_text value "SSQ-112-01-G-S" (at 0 -30.71 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -13.97 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+BATT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "/ESP32-S3-WROOM/GPIO0") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "/ESP32-S3-WROOM/GPIO1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/ESP32-S3-WROOM/GPIO4") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/ESP32-S3-WROOM/GPIO5") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/ESP32-S3-WROOM/GPIO6") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/ESP32-S3-WROOM/GPIO7") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/ESP32-S3-WROOM/GPIO15") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/ESP32-S3-WROOM/GPIO16") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/ESP32-S3-WROOM/GPIO17") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/ESP32-S3-WROOM/GPIO18") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A420)
    (at 105.4 110.2 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Mouser" "200-SSQ10801GS")
    (property "Radiospares" "")
    (property "Sheetfile" "ESP32s3APRS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at -3.4 -10.8 180) (layer "B.SilkS"))
    (fp_text value "SSQ-108-01-G-S" (at 0 -20.55 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -8.89 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VBUS") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/USB Charger/CHGOFF") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/USB Charger/INOKB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/USB Charger/Stat") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/USB Charger/ENBST") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "/USB Charger/Vsys") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:Keystone-1043" locked (layer "B.Cu")
    (tedit 64AC0484)
    (at 158 97 180)
    (property "Mouser" "534-1043")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr through_hole)
    (fp_text reference "J203" (at 27.3 11.3 180) (layer "B.SilkS"))
    (fp_text value "Keystone_1043P" (at 0 0.5 180) (layer "B.Fab") hide)
    (fp_text user "Keystone 1043" (at 0 0.5 180) (layer "B.Fab"))
    (pad "" np_thru_hole circle locked (at 36.11 -7.87 180) (size 2.5 2.5) (drill 2.39) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -27.6 -7.87 180) (size 4 4) (drill 3.55) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 27.6 7.87 180) (size 4 4) (drill 3.55) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at -36.11 0 180) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "input"))
    (pad "2" thru_hole circle locked (at 36.11 0 180) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 61 "Net-(C201-Pad1)") (pinfunction "+") (pintype "input") (zone_connect 2))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 127 100 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "594-NTCS0603E3103FMT")
    (property "Radiospares" "684-1264")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr smd)
    (fp_text reference "TH201" (at 0.3 -1.8) (layer "B.SilkS"))
    (fp_text value "NTC 10K 1% 0603" (at 0 -1.43) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(J204-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:XCVR_L86" locked (layer "B.Cu")
    (tedit 6485DF15)
    (at 185 65 -90)
    (property "Mouser" "277-L86-M33")
    (property "Radiospares" "908-4114")
    (property "Sheetfile" "L86_M33.kicad_sch")
    (property "Sheetname" "L86-M33")
    (attr smd)
    (fp_text reference "U301" (at -10.05 3.45 180) (layer "B.SilkS"))
    (fp_text value "L86-M33" (at -4.1655 -13.279425 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" np_thru_hole circle locked (at -0.6 0.63 270) (size 2.5 2.5) (drill 2.5) (layers F&B.Cu *.Mask))
    (pad "1" smd oval locked (at -7.75 5.85 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "/L86-M33/GPSRX") (pinfunction "RXD1") (pintype "input"))
    (pad "2" smd oval locked (at -7.75 3.31 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "/L86-M33/GPSTX") (pinfunction "TXD1") (pintype "input"))
    (pad "3" smd oval locked (at -7.75 0.77 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" smd oval locked (at -7.75 -1.77 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C301-Pad1)") (pinfunction "VCC") (pintype "input"))
    (pad "5" smd oval locked (at -7.75 -4.31 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "Net-(C303-Pad1)") (pinfunction "V_BCKP") (pintype "input"))
    (pad "6" smd oval locked (at -7.75 -6.85 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "/L86-M33/GPS1PPS") (pinfunction "1PPS") (pintype "input"))
    (pad "7" smd oval locked (at 7.75 -6.85 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "Net-(JP301-Pad2)") (pinfunction "Force") (pintype "input"))
    (pad "8" smd oval locked (at 7.75 -4.31 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/L86-M33/GPSAADET_N") (pinfunction "AADET_N") (pintype "input"))
    (pad "9" smd oval locked (at 7.75 -1.77 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "10" smd oval locked (at 7.75 0.77 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "/L86-M33/GPSRESET") (pinfunction "RESET") (pintype "input"))
    (pad "11" smd oval locked (at 7.75 3.31 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(J301-Pad1)") (pinfunction "EX_ANT") (pintype "input"))
    (pad "12" smd oval locked (at 7.75 5.85 270) (size 2.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "_footprint:BarrelJack_Wuerth_6941xx301002" (layer "B.Cu")
    (tedit 5B191DE1)
    (at 112.6 102.6 90)
    (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
    (tags "connector barrel jack")
    (property "Mouser" "710-694108301002")
    (property "Sheetfile" "MAX77757.kicad_sch")
    (property "Sheetname" "USB Charger")
    (attr through_hole)
    (fp_text reference "J201" (at 0 2.5 90) (layer "B.SilkS"))
    (fp_text value "WR-DC-694108301002" (at 0 -15.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -7.5 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 4.4 1.8) (drill oval 3.4 0.8) (layers *.Cu *.Mask)
      (net 2 "VBUS") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -5.8 90) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 4.8 -3) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_6941xx301002.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 160.8 83.75 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Mouser" "200-HTSW10307GS")
    (property "Radiospares" "180-2117")
    (property "Sheetfile" "ESP32_S3_WROOM.kicad_sch")
    (property "Sheetname" "ESP32-S3-WROOM")
    (attr through_hole)
    (fp_text reference "J501" (at 0.35 2.6 90) (layer "B.SilkS"))
    (fp_text value "HTSW-103-07-G-S" (at 0 -7.41 -90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J501-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(J501-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_footprint:GDEY0213B74_2.13_EPD" (layer "B.Cu")
    (tedit 64B3FE47)
    (at 133.6 65)
    (property "Good Display" "GDEY0213B74")
    (property "Sheetfile" "epd.kicad_sch")
    (property "Sheetname" "E-paper display")
    (attr through_hole)
    (fp_text reference "EPD501" (at 7.7 -0.7) (layer "B.SilkS"))
    (fp_text value "GDEY0213B74" (at 0 0.5) (layer "B.Fab"))
    (fp_text user "GDEY0213B74_2.13_EPD" (at 0 0.5) (layer "B.Fab"))
  )
  (gr_line (start 100 111) (end 100 83) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 199 112) (end 136 112) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 107 82) (end 120.5 82) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 200 83) (end 200 111) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 107 80) (end 141 80) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 100 51) (end 100 54) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 199 50) (end 101 50) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 102 56) (end 102 74) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 200 79) (end 200 51) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 100 76) (end 100 79) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 147 82) (end 193 82) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 147 80) (end 193 80) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 134 110) (end 126 110) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 101 112) (end 124 112) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 134.5 84) (end 122.5 84) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 136.5 82) (end 141 82) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 134 110) (mid 134.707107 110.292893) (end 135 111) (layer "Edge.Cuts") (width 0.05))
  (gr_circle (center 144 81) (end 144 82) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_arc (start 101 55) (mid 100.292893 54.707107) (end 100 54) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 135.5 83) (mid 135.792893 82.292893) (end 136.5 82) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 101 80) (mid 102 81) (end 101 82) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 101 112) (mid 100.292893 111.707107) (end 100 111) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 102 74) (mid 101.707107 74.707107) (end 101 75) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 199 50) (mid 199.707107 50.292893) (end 200 51) (layer "Edge.Cuts") (width 0.05))
  (gr_circle (center 104 81) (end 105 81) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_arc (start 147 82) (mid 146 81) (end 147 80) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 101 80) (mid 100.292893 79.707107) (end 100 79) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 122.5 84) (mid 121.792893 83.707107) (end 121.5 83) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 200 111) (mid 199.707107 111.707107) (end 199 112) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 199 82) (mid 199.707107 82.292893) (end 200 83) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 100 76) (mid 100.292893 75.292893) (end 101 75) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 135.5 83) (mid 135.207107 83.707107) (end 134.5 84) (layer "Edge.Cuts") (width 0.05))
  (gr_circle (center 196 81) (end 196 82) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_arc (start 136 112) (mid 135.292893 111.707107) (end 135 111) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 199 82) (mid 198 81) (end 199 80) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 193 80) (mid 194 81) (end 193 82) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 125 111) (mid 125.292893 110.292893) (end 126 110) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 141 80) (mid 142 81) (end 141 82) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 100 51) (mid 100.292893 50.292893) (end 101 50) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 107 82) (mid 106 81) (end 107 80) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 125 111) (mid 124.719169 111.719169) (end 124 112) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 101 55) (mid 101.707107 55.292893) (end 102 56) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 200 79) (mid 199.707107 79.707107) (end 199 80) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 120.5 82) (mid 121.207107 82.292893) (end 121.5 83) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 100 83) (mid 100.292893 82.292893) (end 101 82) (layer "Edge.Cuts") (width 0.05))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "F.Cu"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "B.Cu"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "B.Paste"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "F.Paste"))
  (gr_text "0V" (at 120.7 108.2) (layer "B.SilkS"))
  (gr_text "AI" (at 185.5 53.6 180) (layer "B.SilkS"))
  (gr_text "PPS" (at 196.2 102.8 -90) (layer "B.SilkS"))
  (gr_text "R1" (at 196.2 100.2 -90) (layer "B.SilkS"))
  (gr_text "T2" (at 185.6 85.7) (layer "B.SilkS"))
  (gr_text "CS" (at 193.1 108.3 180) (layer "B.SilkS"))
  (gr_text "OK" (at 113 108.2) (layer "B.SilkS"))
  (gr_text "Raz" (at 132.1 59.9) (layer "B.SilkS"))
  (gr_text "SQ" (at 188.1 108.3 180) (layer "B.SilkS"))
  (gr_text "DC" (at 195.4 53.6 180) (layer "B.SilkS"))
  (gr_text "ON" (at 190.6 108.3 180) (layer "B.SilkS"))
  (gr_text "On" (at 142.6 110.8 270) (layer "B.SilkS"))
  (gr_text "T1" (at 196.2 98.1 -90) (layer "B.SilkS"))
  (gr_text "SW3" (at 198.3 108.3 180) (layer "B.SilkS"))
  (gr_text "Tool" (at 132.3 61.9) (layer "B.SilkS"))
  (gr_text "AO" (at 190.4 76.4) (layer "B.SilkS"))
  (gr_text "5" (at 161.3 108.2) (layer "B.SilkS"))
  (gr_text "RX" (at 165.9 85.85) (layer "B.SilkS"))
  (gr_text "DC" (at 195.5 108.3 180) (layer "B.SilkS"))
  (gr_text "3v3" (at 132 65.9) (layer "B.SilkS"))
  (gr_text "PTT\n" (at 198 76.4) (layer "B.SilkS"))
  (gr_text "SW3" (at 198.2 53.6 180) (layer "B.SilkS"))
  (gr_text "Bat" (at 180.3 108.3 180) (layer "B.SilkS"))
  (gr_text "ST" (at 115.5 108.2) (layer "B.SilkS"))
  (gr_text "+" (at 130.3 97) (layer "B.SilkS"))
  (gr_text "SW1" (at 182.9 85.7) (layer "B.SilkS"))
  (gr_text "SW2" (at 196.4 55.8 -90) (layer "B.SilkS"))
  (gr_text "ESP32s3APRS\n©️2025 Marc CAPDEVILLE\nCERN-OHL-S v2\ngithub.com/mcapdeville" (at 107.8 90.9 180) (layer "B.SilkS"))
  (gr_text "SD" (at 196.2 90.6 -90) (layer "B.SilkS"))
  (gr_text "0V" (at 183 108.3 180) (layer "B.SilkS"))
  (gr_text "RZ" (at 193 76.4) (layer "B.SilkS"))
  (gr_text "SD" (at 196.4 71.3 -90) (layer "B.SilkS"))
  (gr_text "16" (at 171.5 108.2) (layer "B.SilkS"))
  (gr_text "+" (at 115.9 96.5) (layer "B.SilkS"))
  (gr_text "R1" (at 196.4 61.1 -90) (layer "B.SilkS"))
  (gr_text "7" (at 166.4 108.2) (layer "B.SilkS"))
  (gr_text "Boot" (at 139.5 110.3 -90) (layer "B.SilkS"))
  (gr_text "Off" (at 110.4 108.2) (layer "B.SilkS"))
  (gr_text "HL" (at 196.4 66.2 -90) (layer "B.SilkS"))
  (gr_text "0V" (at 160.8 85.8) (layer "B.SilkS"))
  (gr_text "R2" (at 188 76.4) (layer "B.SilkS"))
  (gr_text "SQ" (at 188 53.6 180) (layer "B.SilkS"))
  (gr_text "ON" (at 190.5 53.6 180) (layer "B.SilkS"))
  (gr_text "SW1" (at 182.8 76.4) (layer "B.SilkS"))
  (gr_text "15" (at 169 108.2) (layer "B.SilkS"))
  (gr_text "0v" (at 131.7 63.9) (layer "B.SilkS"))
  (gr_text "18" (at 176.6 108.2) (layer "B.SilkS"))
  (gr_text "RZ" (at 193.1 85.7) (layer "B.SilkS"))
  (gr_text "SYS" (at 123.2 108.2) (layer "B.SilkS"))
  (gr_text "AI" (at 185.4 108.3 180) (layer "B.SilkS"))
  (gr_text "BST" (at 118 108.2) (layer "B.SilkS"))
  (gr_text "-" (at 185.5 96.5) (layer "B.SilkS"))
  (gr_text "PPS" (at 196.4 58.9 -90) (layer "B.SilkS"))
  (gr_text "PD" (at 196.2 93.1 -90) (layer "B.SilkS"))
  (gr_text "6" (at 163.9 108.2) (layer "B.SilkS"))
  (gr_text "PTT\n" (at 198.1 85.7) (layer "B.SilkS"))
  (gr_text "+" (at 151.1 108.1) (layer "B.SilkS"))
  (gr_text "0" (at 153.8 108.2) (layer "B.SilkS"))
  (gr_text "BU" (at 195.6 85.7) (layer "B.SilkS"))
  (gr_text "0V" (at 182.9 53.6 180) (layer "B.SilkS"))
  (gr_text "0V" (at 180.2 76.4) (layer "B.SilkS"))
  (gr_text "Off" (at 141 110.7 270) (layer "B.SilkS"))
  (gr_text "0V" (at 107.9 108.2) (layer "B.SilkS"))
  (gr_text "SC" (at 196.4 74 -90) (layer "B.SilkS"))
  (gr_text "AO" (at 190.5 85.7) (layer "B.SilkS"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "B.SilkS"))
  (gr_text "HL" (at 196.2 95.7 -90) (layer "B.SilkS"))
  (gr_text "Bat" (at 180.2 53.6 180) (layer "B.SilkS"))
  (gr_text "BUS" (at 105.3 108.2) (layer "B.SilkS"))
  (gr_text "T1" (at 196.4 63.6 -90) (layer "B.SilkS"))
  (gr_text "17" (at 173.9 108.2) (layer "B.SilkS"))
  (gr_text "R2" (at 188.1 85.7) (layer "B.SilkS"))
  (gr_text "T2" (at 185.5 76.4) (layer "B.SilkS"))
  (gr_text "TX" (at 163.35 85.85) (layer "B.SilkS"))
  (gr_text "SC" (at 196.2 88 -90) (layer "B.SilkS"))
  (gr_text "BU" (at 195.5 76.4) (layer "B.SilkS"))
  (gr_text "CS" (at 193 53.6 180) (layer "B.SilkS"))
  (gr_text "0V" (at 180.3 85.7) (layer "B.SilkS"))
  (gr_text "PD" (at 196.4 68.7 -90) (layer "B.SilkS"))
  (gr_text "1" (at 156.3 108.2) (layer "B.SilkS"))
  (gr_text "4" (at 158.8 108.2) (layer "B.SilkS"))
  (gr_text "T" (at 125.4 103.6) (layer "F.SilkS"))
  (gr_text "SC" (at 196.1 88.2 270) (layer "F.SilkS"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "F.SilkS"))
  (gr_text "T1" (at 196.1 98.3 270) (layer "F.SilkS"))
  (gr_text "-" (at 131.1 103.5 180) (layer "F.SilkS"))
  (gr_text "PD" (at 196.1 93.2 270) (layer "F.SilkS"))
  (gr_text "HL" (at 196.1 95.7 270) (layer "F.SilkS"))
  (gr_text "SW2" (at 196.1 106.5 270) (layer "F.SilkS"))
  (gr_text "R1" (at 196.1 100.9 270) (layer "F.SilkS"))
  (gr_text "-" (at 190.8 65.8) (layer "F.SilkS"))
  (gr_text "+" (at 192.7 65.8) (layer "F.SilkS"))
  (gr_text "PPS" (at 196.1 103.5 270) (layer "F.SilkS"))
  (gr_text "+" (at 128.3 103.5 90) (layer "F.SilkS"))
  (gr_text "SD" (at 196.1 90.7 270) (layer "F.SilkS"))
  (gr_text "ESP32s3APRS by F4JMZ\n2/2           V0.0.1\n©️2025 Marc CAPDEVILLE\nLicensed under CERN-OHL-S v2\ngithub.com/mcapdeville/esp32s3aprs" (at 170.2 65.4 270) (layer "B.Mask"))
  (gr_text "ESP32s3APRS by F4JMZ\n1/2           V0.0.1" (at 146.7 84.8) (layer "B.Mask"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "B.Mask"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "F.Mask"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "Dwgs.User"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "Cmts.User"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "B.Fab"))
  (gr_text "Copyright 2025 Marc CAPDEVILLE (F4JMZ)\nThis source describes Open Hardware and is licensed under the CERN-OHL-S v2.\nYou may redistribute and modify this source and make products using it\nunder the terms of the CERN-OHL-S v2 or any later version (https://ohwr.org/cern_ohl_s_v2.txt).\nThis source is distributed WITHOUT ANY EXPRESS OR IMPLIED\nWARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY\nQUALITY AND FITNESS FOR A PARTICULAR PURPOSE. Please see\nthe CERN-OHL-S v2 for applicable conditions.\nAs per CERN-OHL-S v2 section 4, should You produce hardware based\non this source, You must where practicable maintain the Source Location\nvisible on the external case of the products you make using this source." (at 184.3 152.3) (layer "F.Fab"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 200 79.95)
        (xy 100 79.95)
        (xy 100 50)
        (xy 199.95 50)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 200 112)
        (xy 100 112)
        (xy 100 82)
        (xy 200 82)
      )
    )
  )
  (zone (net 61) (net_name "Net-(C201-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 118.1 93.4)
        (xy 119.2 93.4)
        (xy 119.2 95)
        (xy 117.7 95)
        (xy 116.6 93.9)
        (xy 116.6 93.2)
        (xy 116.4 93)
        (xy 115.4 93)
        (xy 115.4 92.6)
        (xy 117.3 92.6)
      )
    )
  )
  (zone (net 88) (net_name "/USB Charger/Vsys") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 122.5 89.4)
        (xy 120.6 89.4)
        (xy 120.6 86.5)
        (xy 122.5 86.5)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C204-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 119.8 89.6)
        (xy 117.9 89.6)
        (xy 117.9 86.5)
        (xy 119.8 86.5)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C204-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 116.1 90)
        (xy 116.1 90.3)
        (xy 116.1 91.2)
        (xy 116.2 91.4)
        (xy 116.2 91.6)
        (xy 116.2 92.3)
        (xy 116.1 92.4)
        (xy 115.3 92.4)
        (xy 114.7 92.4)
        (xy 114.7 91.8)
        (xy 115.3 91.2)
        (xy 115.344672 90.591394)
        (xy 115.45 90.15)
        (xy 115.6 89.8)
        (xy 116 89.8)
      )
    )
  )
  (zone (net 88) (net_name "/USB Charger/Vsys") (layer "F.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 122.6 93.5)
        (xy 121.3 93.5)
        (xy 121 93.2)
        (xy 118.1 93.2)
        (xy 117.3 92.4)
        (xy 116.9 92.4)
        (xy 116.9 91.7)
        (xy 122.6 91.7)
      )
    )
  )
  (zone (net 2) (net_name "VBUS") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 114.2 89.1)
        (xy 114.8 89.7)
        (xy 114.8 90.9)
        (xy 114.7 90.8)
        (xy 114.1 90.8)
        (xy 112.6 89.3)
        (xy 112.6 88.1)
        (xy 114.2 88.1)
      )
    )
  )
  (zone (net 140) (net_name "Diss") (layers F&B.Cu) (name "Dis  SA8x8") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 150.5 67.8)
        (xy 147.9 67.8)
        (xy 147.2 67.1)
        (xy 139.8 67.1)
        (xy 138.6 65.9)
        (xy 138.6 62)
        (xy 139.6 61)
        (xy 150.5 61)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 200 80)
        (xy 100 80)
        (xy 100 50)
        (xy 200 50)
      )
    )
  )
  (zone (net 61) (net_name "Net-(C201-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 118.3 93.3)
        (xy 119.9 94.9)
        (xy 124 94.9)
        (xy 124 99.1)
        (xy 120.8 99.1)
        (xy 119.1 97.4)
        (xy 119.1 96.6)
        (xy 117.1 94.6)
        (xy 117.1 93.3)
      )
    )
  )
  (zone (net 88) (net_name "/USB Charger/Vsys") (layer "B.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 122.6 93.4)
        (xy 118.4 93.4)
        (xy 117.4 92.4)
        (xy 117.4 91.8)
        (xy 120.6 88.6)
        (xy 120.6 86.2)
        (xy 122.6 86.2)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C204-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 119.8 88.5)
        (xy 116.1 92.2)
        (xy 114.7 92.2)
        (xy 114.7 91.6)
        (xy 115.3 91)
        (xy 115.3 90.1)
        (xy 115.3 89.2)
        (xy 118.3 86.2)
        (xy 119.8 86.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.7 80)
        (xy 117.5 80)
        (xy 117.5 76.9)
        (xy 122.7 76.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155 80)
        (xy 149.8 80)
        (xy 149.8 76.9)
        (xy 155 76.9)
      )
    )
  )
  (zone (net 144) (net_name "Dis") (layer "B.Cu") (name "Dis  ESP32") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 174.4 94.6)
        (xy 174.4 98.7)
        (xy 172.5 100.6)
        (xy 165.8 100.6)
        (xy 163 97.8)
        (xy 163 94.5)
        (xy 164.4 93.3)
        (xy 173.1 93.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.9 80)
        (xy 133.7 80)
        (xy 133.7 76.9)
        (xy 138.9 76.9)
      )
    )
  )
)
