<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.635" y1="48.26" x2="49.2" y2="48.26" width="0" layer="20"/>
<wire x1="49.2" y1="48.26" x2="49.2" y2="81.27" width="0" layer="20"/>
<wire x1="49.2" y1="81.27" x2="-0.635" y2="81.27" width="0" layer="20"/>
<wire x1="-0.635" y1="81.27" x2="-0.635" y2="48.26" width="0" layer="20"/>
<hole x="2.54" y="50.8" drill="2.2"/>
<hole x="46.99" y="78.74" drill="2.2"/>
<text>3.3V</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>230V to 5V/3.3V board
Designed by 
Marc-Olivier Schwartz for 
Open Home Automation 
Version 1.0 - 2014</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="myrra">
<packages>
<package name="1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="100nF"/>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="IC1" library="v-reg" package="78XXS" value=""/>
<element name="U$2" library="myrra" package="1" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="GND"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="IN"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="OUT"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="U$2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
