<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>L</text>
<text>N</text>
<wire x1="0" y1="49" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="49" y2="0" width="0" layer="20"/>
<wire x1="49" y1="0" x2="50" y2="1" width="0" layer="20" curve="90"/>
<wire x1="50" y1="1" x2="50" y2="49" width="0" layer="20"/>
<wire x1="50" y1="49" x2="48.8" y2="50" width="0" layer="20" curve="90"/>
<wire x1="48.8" y1="50" x2="1" y2="50" width="0" layer="20"/>
<wire x1="1" y1="50" x2="0" y2="49" width="0" layer="20" curve="90"/>
<hole x="39.5" y="43.8" drill="1.6"/>
<hole x="14.4" y="37.9" drill="1.6"/>
<text>DTR</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<hole x="42.7" y="8.4" drill="1.6"/>
<text>N</text>
<text>L</text>
<text>N</text>
<text>L</text>
<text>MySensors.org</text>
<text>Homini AC Powered 
Relay(2) Module
By Samuel235</text>
<text>Rev1</text>
<text>OpenHardware.io</text>
<text>Relays Rated
@ 2A Each</text>
<wire x1="21.9" y1="46.8" x2="24.7" y2="46.8" width="0" layer="20"/>
<wire x1="24.7" y1="46.8" x2="26" y2="45.8" width="0" layer="20"/>
<wire x1="26" y1="45.8" x2="29.1" y2="45.8" width="0" layer="20"/>
<wire x1="29.1" y1="45.8" x2="29.8" y2="46.8" width="0" layer="20"/>
<wire x1="29.8" y1="46.8" x2="31.5" y2="46.8" width="0" layer="20"/>
<wire x1="31.5" y1="46.8" x2="31.9" y2="46.4" width="0" layer="20" curve="-90"/>
<wire x1="31.9" y1="46.4" x2="31.5" y2="46" width="0" layer="20" curve="-90"/>
<wire x1="31.5" y1="46" x2="30.3" y2="46" width="0" layer="20"/>
<wire x1="30.3" y1="46" x2="29.6" y2="44.9" width="0" layer="20"/>
<wire x1="29.6" y1="44.9" x2="25.8" y2="44.9" width="0" layer="20"/>
<wire x1="25.8" y1="44.9" x2="24.4" y2="46" width="0" layer="20"/>
<wire x1="24.4" y1="46" x2="21.9" y2="46" width="0" layer="20"/>
<wire x1="21.9" y1="46" x2="21.5" y2="46.4" width="0" layer="20" curve="-90"/>
<wire x1="21.5" y1="46.4" x2="21.9" y2="46.8" width="0" layer="20" curve="-90"/>
<wire x1="32.4" y1="38.5" x2="30.5" y2="42.3" width="0" layer="20"/>
<wire x1="29.7" y1="41.9" x2="31.7" y2="38.1" width="0" layer="20"/>
<wire x1="31.7" y1="38.1" x2="32.4" y2="38.5" width="0" layer="20" curve="183.972531"/>
<wire x1="30.5" y1="42.3" x2="29.7" y2="41.9" width="0" layer="20" curve="180"/>
</plain>
<libraries>
<library name="Multicomp_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:01:45</description>
<packages>
<package name="CAPC1608X85N">
</package>
<package name="RESC1608X60N">
</package>
</packages>
</library>
<library name="Fuses">
<packages>
<package name="G5A01072C">
</package>
<package name="C310FC">
</package>
<package name="1206SMD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X06_NO_SILK">
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED 0805&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.0.1 (2015-Apr-26)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://diymodules.org/img/diymodules-lbr-image.php?v=1.0.1" alt="DIYmodules.org"&gt;&lt;/a&gt;&lt;/center&gt;</description>
<packages>
<package name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC-49S-SMT">
</package>
</packages>
</library>
<library name="Relays">
<packages>
<package name="OMRONG3MB-202P">
</package>
</packages>
</library>
<library name="Buttons">
<packages>
<package name="SMD5X5X1.5MM">
</package>
</packages>
</library>
<library name="captain-slow">
<description>Library provided by http://captain-slow.dk/&lt;br&gt;&lt;br&gt;
Find the newest version at https://github.com/blddk/EagleLbr/</description>
<packages>
<package name="HLK-PM01">
</package>
</packages>
</library>
<library name="Ava">
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="Varistors">
<packages>
<package name="14N431K">
</package>
</packages>
</library>
<library name="LD1117">
<packages>
<package name="SOT-223LONG">
</package>
</packages>
</library>
<library name="MOSFETs">
<packages>
<package name="SOT23-2SK3018">
</package>
</packages>
</library>
<library name="Capacitors">
<packages>
<package name="6.3MMSMD">
</package>
</packages>
</library>
<library name="Screwterminals">
<packages>
<package name="5.0MM-SCREWTERMINAL-2-AC">
</package>
</packages>
</library>
<library name="AtmelATSHA204">
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="Board Images">
<packages>
<package name="HIGHVOLTAGEDANGER">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="10uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="22pF">
<attribute name="OC_NEWARK" value="38K9275"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="MPN" value="U0603C220JCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_FARNELL" value="9406107"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="22pF">
<attribute name="OC_NEWARK" value="38K9275"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="MPN" value="U0603C220JCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_FARNELL" value="9406107"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C23" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="4.7uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="F1" library="Fuses" package="G5A01072C" value="TFUSE">
<attribute name="NAME"/>
</element>
<element name="F2" library="Fuses" package="C310FC" value="SFUSE">
<attribute name="NAME"/>
</element>
<element name="ISP2" library="adafruit" package="AVRISP" value="AVRISP-6">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="SW2">
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="NAME"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="SW1">
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="NAME"/>
</element>
<element name="PWR" library="microbuilder" package="CHIPLED_0805" value="Power LED">
<attribute name="NAME"/>
</element>
<element name="LED2" library="microbuilder" package="CHIPLED_0805" value="Relay 1">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="microbuilder" package="CHIPLED_0805" value="Relay 2">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC-49S-SMT" value="8MHz">
<attribute name="NAME"/>
</element>
<element name="R1" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="180R">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R10" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="10K">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="10K">
<attribute name="OC_NEWARK" value="-"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%10K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330399"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="150R">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="150R">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="10K">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="10K">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="SSR1" library="Relays" package="OMRONG3MB-202P" value="OMRON-G3MB">
<attribute name="NAME"/>
</element>
<element name="SSR2" library="Relays" package="OMRONG3MB-202P" value="OMRON-G3MB">
<attribute name="NAME"/>
</element>
<element name="U$2" library="captain-slow" package="HLK-PM01" value="HLK-PM01">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Ava" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="DESCRIPTION" value="8-bit Microcontroller with In-System Programmable Flash"/>
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="NAME"/>
</element>
<element name="VREG2" library="LD1117" package="SOT-223LONG" value="LD1117">
<attribute name="NAME"/>
</element>
<element name="SW1" library="Buttons" package="SMD5X5X1.5MM" value="Reset">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F5" library="Fuses" package="1206SMD" value="2A">
<attribute name="NAME"/>
</element>
<element name="F3" library="Fuses" package="1206SMD" value="2A">
<attribute name="NAME"/>
</element>
<element name="T1" library="MOSFETs" package="SOT23-2SK3018" value="N-Channel Mosfet">
<attribute name="NAME"/>
</element>
<element name="R5" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="10K">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="T2" library="MOSFETs" package="SOT23-2SK3018" value="N-Channel Mosfet">
<attribute name="NAME"/>
</element>
<element name="R7" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="150R">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="150R">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="Capacitors" package="6.3MMSMD" value="100uF">
<attribute name="NAME"/>
</element>
<element name="V2" library="Varistors" package="14N431K" value="250v Varistor">
<attribute name="NAME"/>
</element>
<element name="JP4" library="Screwterminals" package="5.0MM-SCREWTERMINAL-2-AC" value="Device-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="Screwterminals" package="5.0MM-SCREWTERMINAL-2-AC" value="Device-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="Screwterminals" package="5.0MM-SCREWTERMINAL-2-AC" value="AC-INPUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X06_NO_SILK" value="FTDI">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="AtmelATSHA204" package="SOT23-3" value="ATSHA">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-AnalogIC" package="SO08" value="ACS712">
<attribute name="PROD_ID" value="IC-08964"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="1nF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="Multicomp_By_element14_Batch_1" package="CAPC1608X85N" value="0.1uF">
<attribute name="OC_NEWARK" value="37K9922"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="B0603R104KCT"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="OC_FARNELL" value="9406140"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="Multicomp_By_element14_Batch_1" package="RESC1608X60N" value="56K">
<attribute name="OC_NEWARK" value="38K9966"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="MC0.063W06031%15K"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="OC_FARNELL" value="9330615"/>
<attribute name="WATTAGE" value="1/16 W"/>
<attribute name="NAME"/>
</element>
<element name="U$3" library="Board Images" package="HIGHVOLTAGEDANGER" value=""/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="M2" library="diy-modules" package="WIRELESS-NRF24L01" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="VREG2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="PWR" pad="C"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="ISP2" pad="6"/>
<contactref element="C23" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="T2" pad="S"/>
<contactref element="T1" pad="S"/>
<contactref element="C8" pad="2"/>
<contactref element="U$2" pad="VO-"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="M2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C7" pad="2"/>
<contactref element="VREG2" pad="3"/>
<contactref element="C11" pad="2"/>
<contactref element="SSR1" pad="+"/>
<contactref element="R3" pad="1"/>
<contactref element="SSR2" pad="+"/>
<contactref element="R4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="U$2" pad="VO+"/>
<contactref element="C8" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="INPUT_LIVE">
<contactref element="F2" pad="1"/>
<contactref element="SSR2" pad="LOAD1"/>
<contactref element="JP8" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="F2" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="AC_L"/>
<contactref element="V2" pad="2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="INPUT_NEUTRAL">
<contactref element="U$2" pad="AC_N"/>
<contactref element="V2" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="VREG2" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="ISP2" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="M2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="D12_MISO">
<contactref element="U1" pad="16"/>
<contactref element="ISP2" pad="1"/>
<contactref element="M2" pad="7"/>
</signal>
<signal name="D11_MOSI">
<contactref element="U1" pad="15"/>
<contactref element="ISP2" pad="4"/>
<contactref element="M2" pad="6"/>
</signal>
<signal name="D13_SCK">
<contactref element="U1" pad="17"/>
<contactref element="ISP2" pad="3"/>
<contactref element="M2" pad="5"/>
</signal>
<signal name="D10_CSN">
<contactref element="U1" pad="14"/>
<contactref element="M2" pad="4"/>
</signal>
<signal name="D9_CE">
<contactref element="U1" pad="13"/>
<contactref element="M2" pad="3"/>
</signal>
<signal name="D2_INQ">
<contactref element="U1" pad="32"/>
<contactref element="M2" pad="8"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="ISP2" pad="5"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="DTR">
<contactref element="C5" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="31"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="30"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="20"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="Q1" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="Q1" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D3_RELAY1">
<contactref element="U1" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D4_RELAY2">
<contactref element="U1" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="LOADL">
<contactref element="SSR1" pad="LOAD2"/>
<contactref element="F5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="SSR1" pad="-"/>
<contactref element="LED2" pad="C"/>
<contactref element="T1" pad="D"/>
</signal>
<signal name="N$8">
<contactref element="F5" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED3" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="LOADL1">
<contactref element="SSR2" pad="LOAD2"/>
<contactref element="F3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="SSR2" pad="-"/>
<contactref element="LED3" pad="C"/>
<contactref element="T2" pad="D"/>
</signal>
<signal name="N$12">
<contactref element="F3" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="D5_SWITCH1">
<contactref element="U1" pad="9"/>
<contactref element="JP7" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D6_SWITCH2">
<contactref element="U1" pad="10"/>
<contactref element="R10" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="T1" pad="G"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="T2" pad="G"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="6"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="SENSE_LIVE">
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="4"/>
<contactref element="SSR1" pad="LOAD1"/>
</signal>
<signal name="A3_ATSHA">
<contactref element="U1" pad="26"/>
<contactref element="U2" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="A2_SENSE">
<contactref element="U1" pad="25"/>
<contactref element="U$1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
