<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<text>V2.1</text>
<text>2017/12</text>
<hole x="2.821" y="2.8194" drill="3.5"/>
<hole x="41.6306" y="41.529" drill="3.5"/>
<hole x="2.821" y="41.529" drill="3.5"/>
<hole x="41.6306" y="2.8194" drill="3.5"/>
<wire x1="18.261" y1="-1.189" x2="26.262" y2="-1.189" width="0.127" layer="20"/>
<wire x1="26.262" y1="-1.189" x2="27.278" y2="-0.173" width="0.127" layer="20"/>
<wire x1="44.75" y1="3.683" x2="44.75" y2="40.767" width="0.127" layer="20"/>
<wire x1="44.75" y1="40.767" x2="40.894" y2="44.623" width="0.127" layer="20" curve="90"/>
<wire x1="40.894" y1="44.623" x2="3.556" y2="44.623" width="0.127" layer="20"/>
<wire x1="3.556" y1="44.623" x2="-0.3" y2="40.467" width="0.127" layer="20" curve="90"/>
<wire x1="-0.3" y1="40.467" x2="-0.3" y2="3.383" width="0.127" layer="20"/>
<wire x1="-0.3" y1="3.383" x2="3.556" y2="-0.173" width="0.127" layer="20" curve="90"/>
<wire x1="17.245" y1="-0.173" x2="18.261" y2="-1.189" width="0.127" layer="20"/>
<wire x1="44.75" y1="3.683" x2="40.894" y2="-0.173" width="0.127" layer="20" curve="-90"/>
<wire x1="3.556" y1="-0.173" x2="17.245" y2="-0.173" width="0.127" layer="20"/>
<wire x1="40.894" y1="-0.173" x2="27.278" y2="-0.173" width="0.127" layer="20"/>
<text>GND</text>
<text>SWITCH BOARD</text>
<text>TOUCH</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="TD-MySensors">
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="NCA_Sensors">
<packages>
<package name="SOT-23-6">
</package>
</packages>
</library>
<library name=",giltesa">
<packages>
<package name="LED_RGB_1206_SIDE">
</package>
<package name="NRF24L01_SMD">
</package>
<package name="JST-8-1MM-SMD">
</package>
<package name="2X4_SMD_2.0MM">
</package>
<package name="HTTM_SENSEPAD">
</package>
<package name="R0603">
</package>
<package name="C0603">
</package>
<package name="C1206">
</package>
</packages>
</library>
<library name=",giltesa_logos">
<packages>
<package name="MYSENSORS">
</package>
<package name="DOMOTICA-10MM">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
<library name="MySMD2">
<packages>
<package name="RESONATOR">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library=",giltesa" package="R0603" value="10K">
<attribute name="VALUE"/>
</element>
<element name="C1" library=",giltesa" package="C1206" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="U2" library="TD-MySensors" package="SOT23-3" value="ATSHA204A">
<attribute name="VALUE"/>
</element>
<element name="C7" library=",giltesa" package="C0603" value="100nF"/>
<element name="TTP1" library="NCA_Sensors" package="SOT-23-6" value="TTP223">
<attribute name="VALUE"/>
</element>
<element name="C8" library=",giltesa" package="C0603" value="0-50pF">
<attribute name="VALUE"/>
</element>
<element name="C9" library=",giltesa" package="C0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="EIA3216" value="100uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library=",giltesa_logos" package="MYSENSORS" value="MYSENSORS"/>
<element name="LOGO1" library="ohw-logo" package="OSHW_FILLX150_NOTEXT" value="OSHW_LOGO_FILLX0150-NT"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE" value="ATMEGA328P_TQFP"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library=",giltesa" package="C0603" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="MySMD2" package="RESONATOR" value="8MHz">
<attribute name="VALUE"/>
</element>
<element name="C2" library=",giltesa" package="C0603" value="100nF"/>
<element name="L1" library=",giltesa" package="LED_RGB_1206_SIDE" value="LED_RGB"/>
<element name="Q1" library="SparkFun" package="SOT23" value="MMBT2222">
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun" package="SOT23" value="MMBT2222">
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun" package="SOT23" value="MMBT2222">
<attribute name="NAME"/>
</element>
<element name="RR1" library="SparkFun-Passives" package="0603-ARV" value="1K">
<attribute name="VALUE"/>
</element>
<element name="U$5" library=",giltesa_logos" package="DOMOTICA-10MM" value="DOMOTICA-10MM"/>
<element name="RR2" library="SparkFun-Passives" package="0603-ARV" value="10K">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$7" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$14" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="R1" library=",giltesa" package="R0603" value="68R">
<attribute name="VALUE"/>
</element>
<element name="U$8" library=",giltesa" package="NRF24L01_SMD" value="NRF24L01">
<attribute name="VALUE"/>
</element>
<element name="FLASH" library="SparkFun-DigitalIC" package="SO08" value="SPI_FLASH-W25X40CLSNIG">
<attribute name="NAME"/>
</element>
<element name="R10" library=",giltesa" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="JST1" library=",giltesa" package="JST-8-1MM-SMD" value="AVRISP+UART">
<attribute name="VALUE"/>
</element>
<element name="J3" library=",giltesa" package="2X4_SMD_2.0MM" value="2X4_SMD_2.0MM"/>
<element name="U$1" library=",giltesa" package="HTTM_SENSEPAD" value="HTTM_SENSEPAD"/>
<element name="R3" library=",giltesa" package="R0603" value="10R">
<attribute name="VALUE"/>
</element>
<element name="R4" library=",giltesa" package="R0603" value="10R">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="TTP1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C4" pad="C"/>
<contactref element="C5" pad="C"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="Y1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="RR2" pad="3"/>
<contactref element="RR2" pad="4"/>
<contactref element="RR2" pad="2"/>
<contactref element="U$8" pad="GND"/>
<contactref element="FLASH" pad="4"/>
<contactref element="JST1" pad="2"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="RR2" pad="8"/>
<contactref element="JST1" pad="4"/>
</signal>
<signal name="D9_LEDR~">
<contactref element="U1" pad="13"/>
<contactref element="RR1" pad="1"/>
</signal>
<signal name="D10_LEDG~">
<contactref element="U1" pad="14"/>
<contactref element="RR1" pad="2"/>
</signal>
<signal name="D13_SCK">
<contactref element="U1" pad="17"/>
<contactref element="U$8" pad="SCK"/>
<contactref element="FLASH" pad="6"/>
<contactref element="JST1" pad="6"/>
</signal>
<signal name="D11_MOSI">
<contactref element="U1" pad="15"/>
<contactref element="U$8" pad="MOSI"/>
<contactref element="FLASH" pad="5"/>
<contactref element="JST1" pad="5"/>
</signal>
<signal name="D12_MISO">
<contactref element="U1" pad="16"/>
<contactref element="U$8" pad="MISO"/>
<contactref element="FLASH" pad="2"/>
<contactref element="JST1" pad="3"/>
</signal>
<signal name="A3_ATSHA204A">
<contactref element="U2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="D2_TS1">
<contactref element="TTP1" pad="1"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="D0_RX">
<contactref element="U1" pad="30"/>
<contactref element="JST1" pad="7"/>
</signal>
<signal name="D1_TX">
<contactref element="U1" pad="31"/>
<contactref element="JST1" pad="8"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$33">
<contactref element="U1" pad="20"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="Y1" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="1"/>
<contactref element="RR1" pad="8"/>
<contactref element="RR2" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="L1" pad="RED"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="1"/>
<contactref element="RR1" pad="7"/>
<contactref element="RR2" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="Q3" pad="1"/>
<contactref element="RR1" pad="6"/>
<contactref element="RR2" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="1"/>
<contactref element="L1" pad="BLUE"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="D5_SSR1~">
<contactref element="J3" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="+5V">
<contactref element="J3" pad="6"/>
</signal>
<signal name="D6_SSR2~">
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="+3V3">
<contactref element="J3" pad="8"/>
<contactref element="C4" pad="A"/>
<contactref element="C5" pad="A"/>
<contactref element="FLASH" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="FLASH" pad="8"/>
<contactref element="FLASH" pad="7"/>
<contactref element="L1" pad="VCC"/>
<contactref element="TTP1" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$8" pad="3.3V"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="RR2" pad="1"/>
<contactref element="JST1" pad="1"/>
</signal>
<signal name="D3_H11AA1">
<contactref element="J3" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="A1_DS18B20">
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="A0_SS_FLASH">
<contactref element="FLASH" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="D7_CE">
<contactref element="U$8" pad="CE"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="D8_CSN">
<contactref element="U$8" pad="CSN"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="D4_LEDB">
<contactref element="RR1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q3" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="SENSEPAD"/>
<contactref element="TTP1" pad="3"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="1"/>
<contactref element="L1" pad="GREEN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
