<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="-10.5985" y1="10.5985" x2="-10.5985" y2="-10.5985" width="0.2032" layer="20" curve="90"/>
<wire x1="-10.5985" y1="-10.5985" x2="10.5985" y2="-10.5985" width="0.2032" layer="20" curve="90"/>
<wire x1="10.5985" y1="-10.5985" x2="10.5985" y2="10.5985" width="0.2032" layer="20" curve="90"/>
<wire x1="10.5985" y1="10.5985" x2="-10.5985" y2="10.5985" width="0.2032" layer="20" curve="90"/>
<wire x1="-20.1" y1="20.1" x2="-20.1" y2="-20.1" width="0.2032" layer="20" curve="90"/>
<wire x1="-20.1" y1="-20.1" x2="20.1" y2="-20.1" width="0.2032" layer="20" curve="90"/>
<wire x1="20.1" y1="-20.1" x2="20.1" y2="20.1" width="0.2032" layer="20" curve="90"/>
<wire x1="-20.1" y1="20.1" x2="-20.066" y2="57.023" width="0.2032" layer="20"/>
<wire x1="-20.066" y1="57.023" x2="20.066" y2="57.023" width="0.2032" layer="20"/>
<wire x1="20.066" y1="57.023" x2="20.1" y2="20.1" width="0.2032" layer="20"/>
<text>V1.0</text>
<text>2018/06</text>
<hole x="20.32" y="-10.795" drill="2.54"/>
<hole x="-20.32" y="-10.795" drill="2.54"/>
<hole x="15.875" y="24.495" drill="2.54"/>
<hole x="-15.875" y="24.495" drill="2.54"/>
<hole x="0" y="53.975" drill="2.54"/>
<text>12V</text>
<text>ANDONSTAR LED RING 30MM</text>
<text>RT 1L*</text>
</plain>
<libraries>
<library name=",giltesa">
<packages>
<package name="LED_Z_POWER">
</package>
<package name="R0603">
</package>
<package name="R1206">
</package>
<package name="C0603">
</package>
<package name="TO-252">
</package>
<package name="1X03_SMD">
</package>
<package name="TRIMPOT_SMD_16MM">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="cc-by-nc-sa">
<packages>
<package name="CC-NC-B_NIX">
</package>
</packages>
</library>
<library name=",giltesa_logos">
<packages>
<package name="GILTESA.COM_MASK">
</package>
<package name="GILTESA.COM_COPPER_STOP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SO08">
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="GF1">
<description>&lt;b&gt;GF1&lt;/b&gt;&lt;p&gt;
General Semiconductor</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Amplifiers">
<description>&lt;h3&gt;SparkFun Amplifiers&lt;/h3&gt;
This library contains analog amplifiers, mostly operational amplifiers but also has some headphone and audio amps with more specific applications.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;Op-amps&lt;/li&gt;
&lt;li&gt;Headphone amps&lt;/li&gt;
&lt;li&gt;Class D amps&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L6" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="L5" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="L4" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="L3" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="L2" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="L1" library=",giltesa" package="LED_Z_POWER" value="1W">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="ohw-logo" package="OSHW_FILLX150_NOTEXT" value="OSHW_LOGO_FILLX0150-NT"/>
<element name="U$6" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$7" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$14" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$20" library="cc-by-nc-sa" package="CC-NC-B_NIX" value="CC-NC-BCNIX"/>
<element name="U$1" library=",giltesa_logos" package="GILTESA.COM_MASK" value="GILTESA.COM_MASK"/>
<element name="IC1" library="adafruit" package="SO08" value="NE555">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library=",giltesa" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library=",giltesa" package="R0603" value="910R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library=",giltesa" package="R0603" value="910R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library=",giltesa" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library=",giltesa" package="R1206" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library=",giltesa" package="C0603" value="700nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library=",giltesa" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="GF1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="linear" package="SOT89" value="78L05F">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G1" library=",giltesa" package="TO-252" value="N310AD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Amplifiers" package="SO08" value="LM358">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R2512" value="10R 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R2512" value="10R 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="adafruit" package="DCJACK_2MM_SMT" value="2.1MMJACKSMT"/>
<element name="TM" library=",giltesa" package="1X03_SMD" value="">
<attribute name="VALUE"/>
</element>
<element name="U$8" library=",giltesa_logos" package="GILTESA.COM_COPPER_STOP" value="GILTESA.COM_COPPER_STOP"/>
<element name="R8" library=",giltesa" package="TRIMPOT_SMD_16MM" value="10K*">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="L6" pad="A"/>
<contactref element="L5" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="L5" pad="A"/>
<contactref element="L4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="L3" pad="A"/>
<contactref element="L2" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="L2" pad="A"/>
<contactref element="L1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="VR1" pad="2"/>
<contactref element="VR1" pad="2@1"/>
<contactref element="G1" pad="S"/>
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="A"/>
<contactref element="L4" pad="A"/>
<contactref element="L1" pad="A"/>
<contactref element="U$2" pad="PWR2"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="3"/>
<contactref element="TM" pad="2"/>
<contactref element="R8" pad="S"/>
</signal>
<signal name="N$21">
<contactref element="VR1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="VR1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="8"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$26">
<contactref element="G1" pad="G"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R5" pad="1"/>
<contactref element="TM" pad="3"/>
<contactref element="R8" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="R4" pad="2"/>
<contactref element="TM" pad="1"/>
<contactref element="R8" pad="B"/>
</signal>
<signal name="N$5">
<contactref element="L3" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="L6" pad="C"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="G1" pad="D"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
